| # Physical Breakdowns (tscfg2110m000) Use this session to maintain physical breakdowns. A physical breakdown is defined for an Installation, and enables you to view the configuration's build-up structure and as-maintained structure. Only the serialized items that are currently installed in the configuration or Installment, are displayed in the physical breakdown. You can view the removed serialized items in the Physical Breakdown Log (tscfg2515m000) session. Note If the Functional Elements Active check box in the General Service Parameters (tsmdm0100m000) session is selected, you can use functional elements in physical breakdowns. If you view the physical breakdown through the graphical browser framework, note that LN also uses the data entered in the Physical Breakdown Log (tscfg2515m000) session. The Replace Serial Number command that starts the Replace Serial Number (tscfg2210m800) session allows you to replace the old serial number with the new serial number, is displayed only when you select the Configuration Status Usage checkbox in the Configuration Management Parameters (tscfg0100m000) session. Related topics To maintain physical breakdowns Installation group layout example To use functional elements Parent Item The item code of the parent serialized item. Note The parent serialized item cannot be a lot item. Serial Number The serial number of the parent serialized item. Description The description or name of the parent serialized item. Revision The identification of any revisions of serialized items. Installation Group The code of the installation group to which the parent serialized item (and therefore, all of its child items) belongs. Description The description or name of the code. Owner The name of the business partner who owns the parent and child serialized items. Position The position number of the child item or child component in the physical breakdown of the parent item. Related topics Numbering Parent Item Picture The serialized item picture, defaulted from the Serialized Items (tscfg2100m000) session. If the picture is not available in the Serialized Items (tscfg2100m000) session, the picture is defaulted from the Item - General (tcibd0101s000) session. Note If you access the details of a particular line, the picture of the serialized child items is displayed. If the picture is not present in the Serialized Items (tscfg2100m000) session, the serialized child item picture is defaulted from the Items - General (tcibd0501m000) session. Item The item code of the child item. Related topics To define serialized items Serial Number The serial number of the child serialized item. This number can be the serial number of a lot item. Note A child serialized-item can occur only once in the breakdown. The child serialized item and the parent serialized item cannot be the same in one physical breakdown. The Status field is disabled if the serial number is not entered. Description The description or name of the child item. Revision The identification of any revisions of serialized items. Quantity The quantity of the child item in the physical breakdown of the parent item. Note If the serial number is filled, this field displays 1 (one) and is disabled. Quantity The unit used to express the quantity of the child item. Functional Element The functional element group that the child item belongs to. Note Functional elements can only be defined if the Functional Elements Active check box in the General Service Parameters (tsmdm0100m000) session is selected. You cannot change the functional element in a physical breakdown. A parent item and child item combination can only belong to one functional element. Related topics To use functional elements Reference Designator Reference Designator Related topics Overview of reference designators. Description The description or name of the code. This can be, for example, a code that expresses the location where you must mount a component item. Structure Type The type of physical breakdown structure defined for the item. LN does not allow you to install an item with Structure Type set to Structure as a child of a physical item. Allowed values Structure Type Note This field is visible only if the Structure Type Usage check box is selected in the Configuration Management Parameters (tscfg0100m000). Status The Status of the (serialized) item in the physical breakdown. Note The status cannot be changed manually. Status Start Time The date on which the status was set or last changed. Clear Dummy Serial Field Clears the Dummy Serial Number field for the item and its physical breakdown structure. Create Physical Breakdown Starts the Physical Breakdowns (tscfg2110m000) session. From As-built Structure... You can create a physical breakdown structure from an as-built structure. From Item Breakdown... You can create a physical breakdown structure from an item breakdown. Create Physical Breakdown Structure from ASCII-File You can create a physical breakdown structure from an ASCII file. Copy Project Breakdown Structure You can create a physical breakdown structure from a project-breakdown structure. Replace Starts the Change Physical Breakdown (tscfg2220m000) session. You can replace the item in this session. Install Starts the Change Physical Breakdown (tscfg2220m000) session. You can install the item in this session. Remove Starts the Change Physical Breakdown (tscfg2220m000) session. You can remove the item in this session. Level Up Displays the parent item one level up. If the current parent item is the item on the highest level in the breakdown, this command is disabled. Level Down Displays the components of a child item in the current breakdown. You must first select a line in the breakdown to enable this command. View Tree Displays the structure of the selected physical breakdown in a graphical way. View Log Displays the physical breakdown logs. Item Details Displays the details of the serialized items. View Alternate Items Displays alternate items. Delete Physical Breakdown Deletes the physical breakdown. |