| # Costing breaks in Manufacturing Costing breaks in Manufacturing Costing breaks are defined to override a project peg distribution of actual supply orders and move the related costs to different WBS levels on the same project. In the bill of material (BOM), costing breaks can be applied to routings, operations, work centers, or cost types. Multiple costing breaks can be applied to a specific BOM. New field by session The Project Peg Origin field is added to these sessions: Operation Cost Distribution (ticst0503m000) Estimated Material Distribution (ticst0508m000) Material to Issue Distribution (ticst0508m001) Operation Cost Distribution History (ticst1558m000) Production Order Distribution (tisfc0105m000) Production Order Distribution (tisfc0105m100) Project Peg - Production Orders (tisfc0105m300) Related topics Costing Breaks Costing Breaks in Enterprise Planning and Manufacturing Project Pegging Costing Breaks in Depot Repair Service Costing Break Hierarchy and Search Path |