| # Print Work Instructions (tiasc5450m000) Use this session to print the work instructions for line-station orders. Related topics Assembly control overview Assembly orders Assembly Line A set of consecutive line stations in which FAS (Final Assembly Schedule) items are manufactured. The items are manufactured by passing the items from line station to line station and by carrying out operations at each line station. An assembly line is subdivided into a number of line segments separated by buffers. An assembly line can be either a main line or a supplying line. Line Segment A set of consecutive assembly-line work centers on an assembly line between two buffers. The first buffer is the beginning of the segment, the next buffer is the first part of the next segment. Reference Date Line stations are date-effective. Select the date when you want the line stations to be valid. The reference date is also used to check which line stations are valid in ASC. Sort Select the report layout you require. To preview the layout, take the following steps: Select the relevant record(s) Click Print Type D in the Device field. Click Continue For a complete list of the contents of the work instructions, see the Complete List of Work Instructions, listed previously. Print What Work instructions include, among others, options, operations, assembly parts, instructions, and tasks. For a complete list of the contents of the work instructions, see the previous list. Originals Print work instructions that have not already been printed and have a Line Station Order Status from Planned to Closed. Reprint Print work instructions that have already been printed for line-station orders that have a Line Station Order Status from Frozen to Closed. Differences Only Only the differences are printed. Specifically, only the changes made since the first printing after the order has been frozen. Differences can only be printed for line station orders that have the status Frozen or Closed. Note You can change the content of an order after a line station variant, which is linked to the order, is made order-specific, when the order is frozen. The changes that are made, can be applied after the work instructions have been printed. Print Prints the entered selection. |