| # Physical Breakdown Log (tscfg2515m000) Use this session to display the installations and / or removals of child items to / from a serialized item's physical breakdown. Note The installations or removals are logged automatically, but only if both of the following conditions are met: The serialized item's status in the Serialized Items (tscfg2100m000) session is Active. In the Configuration Management Parameters (tscfg0100m000) session, either the Configuration Status Usage check box or the Create Physical Breakdown Log check box is selected. The graphical browser framework (GBF) that you can start in the Physical Breakdowns (tscfg2110m000) session, also uses the data in this session. Related topics Updating Physical Breakdown Structure Approve-Reject changes & Update Physical Breakdown Superseded Serialized Items Parent Item The item code of the parent serialized item, for which changes to its physical breakdown are logged and displayed in this session. Serial Number The serial number of the parent item whose physical breakdown changes are logged and now displayed in this session. Description Description or name of the item. Revision The identification of any revisions of the serialized item. Installation Group The code of the installation group that the parent serialized item belongs to. Description The description or name of the code. Owner The name of the business partner who owns the parent and child serialized items. Position The position number of the child item or child component in the breakdown. Changed By The name of the user that initiated the changes made to a component of a physical breakdown structure. Note This is a display field. Infor LN defaults the value in this field. Source of Change The source that initiated the changes made to a component of a physical breakdown structure. Allowed values Source of Change Note This is a display field. Infor LN defaults the value in this field. By default, the value in this field is set to Not Applicable. Order Number The order number that initiated the changes made to a component of a physical breakdown structure. Note This field is applicable only if the value of the Source of Change field is set to Maintenance Sales Order or Work Order or Service Order. This is a display field. Infor LN defaults the value in this field. Effectuation Time The date the child item was either removed from, or installed in, the parent item's physical breakdown, using the Change Physical Breakdown (tscfg2220m000) session. Status The status that the child item was changed to in the physical breakdown. Item The item code of the child item that was either removed from, or installed in, the physical breakdown. Serial Number The serial number of the child item that was either removed from or installed in the parent item's physical breakdown. Description The name or description of the child item. Quantity The number of child items in the physical breakdown. Note If the serial number is filled, this field must be 1 (one). No Help topic is associated with this item. Quantity The inventory unit of the item. Reference Designator Indicates the location to insert a component on an item, for example, where to mount an electronic component on a Printed Circuit Board. Reference designators are often used in electronics, and can originate from a Computer-Aided Design (CAD) station. Related topics Overview of reference designators Description The description or name of the code. This can be, for example, a code that expresses the location where you must mount a component item. Level &Up Use this command to display the parent item one level up. If the current parent item is the item on the highest level in the breakdown, this command is disabled. Level &Down Use this command to display the components of a child item in the current breakdown. You must first select a line in the breakdown to enable this command. |