| # Displaying MBC A list of previously defined MBCs is displayed . To define a new MBC: Click New To modify an MBC: Double-click the MBC You can only modify MBCs that have the In Design status. To use MBCs You can apply an MBC in two situations: To change and approve a number of EBOMs. For more information, refer to Changing EBOMs - Automatic procedure To approve the changes in a number of EBOMs, after you made changes in the EBOMs manually. For more information, refer to Changing EBOMs - Semi-automatic procedure. If the Manual Revision Numbering check box in the Engineering Data Management Parameters (tiedm0100m000) session is selected, finalizing an MBC procedure is different in some respects. For more information, refer to the field Help. MBC Definition You can use the following sessions to define the effects of an MBC: MBC Action (tiedm3120m000) Include/Exclude E-Items (tiedm3121m000) E-Item by MBC (tiedm3122m000) MBC simulation If you select one or more MBCs, and click Simulate ... or Simulate (Detailed)... on the appropriate menu, you can produce a report that shows the effects of the MBCs. To select nonadjacent MBCs, hold down the CTRL key while you click the MBC. MBCs and reference designators You can use actions that are linked to an MBC to add, delete, or replace reference designators in EBOMs. For more information, refer to Reference designators and MBCs. Related topics Changing EBOMs - Automatic procedure Changing EBOMs - Semi-automatic procedure Engineering data management summary Reference designators and MBCs |