| # Print Remix/Sequence Parameters (tiasl4410m000) Use this session to print details of the sequencing parameters for a range of users and a range of line segments. During sequencing, the parameters of a line segment are used when that segment is the pivot segment. During mixing, you have to specify from which segment the parameters are taken. Note You can define more general parameters in the Assembly Control Parameters (tiasc0100m000) session. Related topics Line sequencing and rule types in Assembly Control Assembly control overview Print Prints the entered selection. |