| # Master Loads (fmlbd4510m000) Use this session to view master loads. A master load is a group of loads that travel a route plan. Related topics The use of route plans The load building process Load plan, load, and shipment maintenance Plan The load plan to which the master load belongs. Master Load The master load. A master load is a group of loads that travel the same route plan. Load A load that belongs to the master load. Shipment A shipment of the load that belongs to the master load. Shipment Line The shipment line number of the shipment. Trip The trip on which the shipment is based. Route Plan A network of loading and unloading addresses, one of which is a pooling point. A route plan is usually defined for routes that involve multi-modal transport. A route plan consists of one or more legs. Each leg, or part of the route, can be handled differently depending on the specified transport category and transport means group. Route Plan Leg The advance leg is the first part of the route where goods are picked up and transported to a pooling point, such as an airport, a train station, or a port. The main leg starts at the pooling point and ends at the intermediate destination. At the pooling point, the goods from the advance leg are loaded into an aircraft, ship, train, or truck, and brought to the intermediate destination. The beyond leg spans the intermediate destination and the final destination. At the intermediate destination, the goods are transferred from the airplane to trucks to bring the goods to their final destination. A route plan may consist of more than one advance and beyond legs, but one main leg. The first leg that you define is always of the main type. Route Plan Line The identifying number of the route plan leg. Route Plan Sequence The sequence number of an advance or beyond leg. The sequence number indicates the order in which the addresses along the route plan legs are called at. Freight Order Line The freight order from which the loads of the master load are created. Freight Order Line The freight order line from which the loads of the master load are created. |