| # Print Quality Combinations (qmptc0411m000) Use this session to print (a range of) quality combinations. Origin An integrated module or package to which an (inspection) order is related. Quality inspections are executed within a module or package. This field is used to select one of the implemented modules or packages of LN. See also: Origin of Inspection Note In the Quality Management Parameters (qmptc0100m000) session you can maintain the implemented modules and packages. From Item item To Item item From Sub-Item A means to further classify items. A sub-item can either be: A component item used in a bill of material. A material used in a formula. To Sub-Item A means to further classify items. A sub-item can either be: A component item used in a bill of material. A material used in a formula. Quality Group quality group Quality Group quality group Line The component's BOM position number. Line The component's BOM position number. Business Partner business partner Business Partner business partner Routing The sequence of operations required to manufacture an item. For each operation, the task, machine, and work center are specified, as well as information about setup time and cycle time. Routing The sequence of operations required to manufacture an item. For each operation, the task, machine, and work center are specified, as well as information about setup time and cycle time. Operation One of a series of steps in a routing that are carried out successively to produce an item. The following data is collected during a routing operation: The task. For example, sawing. The machine used to carry out the task (optional). For example, sawing machine. The place where the task is carried out (work center). For example, woodwork. The number of employees required to carry out the task. This data is used to compute order lead times, to plan production orders and to calculate cost prices. Operation One of a series of steps in a routing that are carried out successively to produce an item. The following data is collected during a routing operation: The task. For example, sawing. The machine used to carry out the task (optional). For example, sawing machine. The place where the task is carried out (work center). For example, woodwork. The number of employees required to carry out the task. This data is used to compute order lead times, to plan production orders and to calculate cost prices. Task An activity to manufacture or repair an item. For example, sawing, drilling, or painting. A task is carried out on a work center, and can be related to a machine. Task An activity to manufacture or repair an item. For example, sawing, drilling, or painting. A task is carried out on a work center, and can be related to a machine. From Warehouse warehouse From Warehouse warehouse To Warehouse warehouse To Warehouse warehouse Quality ID The code to which data is linked that is necessary to check the quality requirements of an item. Since one standard test procedure can be used for a group of products that require the same quality standards and tests, a standard test procedure can considerably reduce time. Quality ID The code to which data is linked that is necessary to check the quality requirements of an item. Since one standard test procedure can be used for a group of products that require the same quality standards and tests, a standard test procedure can considerably reduce time. Print Text If this check box is selected, the text that is linked to the quality combinations (defined in the Quality Combinations (qmptc0111m000) session) is printed in the report. |