| # Import component data To import master data for DEM (the so-called component data) complete the following steps: Start the Import Component Model Data (tgbrg5256m000) session. On the Settings tab, specify the following values: File: <Temp Directory>component_90_20090929.cmp.Z Print Errors: Select. Overwrite: Clear. Components From: space. To: zzzzz, which is the maximum value. Component Releases From: space, To: zzzzz, which is the maximum value. Applications: select. From: space. To: zzzzz, which is the maximum value. Subapplications: Select. Do not overwrite Texts Within: Clear all. Import Application Conversion Data: Clear. On the Application Conversion Data tab, specify the following values: Source Component From: space. To: zzzzz, which is the maximum value. Source Component Release From: space. To: zzzzz, which is the maximum value. Source Application From: space. To: zzzzz, which is the maximum value. Destination Component From: space. To: zzzzz, which is the maximum value. Destination Component Release From: space. To: zzzzz, which is the maximum value. Destination Application From: space. To: zzzzz, which is the maximum value. Do Not Overwrite Texts Within: select. Click Import. |