| # Physical Breakdown Changes (tscfg2140m000) Use this session to view the set of changes made to the physical breakdown structure. The changes can be made at the parent item level and/or at the component level. The changes are registered using a unique Change Number. This session maintains the details of the Parent Item (serialized) to which the changes are made. If the existing serialized item is superseded, this session maintains the details of the New Item and the New Serial Number. If the changes are related to an order, the Order Type and the Order Number are also maintained in this session. Note This session is visible only if the Physical Breakdown Changes check box is selected in the Configuration Management Parameters (tscfg0100m000) session. Related topics Updating Physical Breakdown Structure Approve-Reject changes & Update Physical Breakdown Superseded Serialized Items Parent Item The code of the parent serialized item. The changes are applied to the components of this Parent Item. Note This item must be specified in the Item field and the Configuration Controlled field must be set to Serialized in the Items - Service (tsmdm2100m000) session. Parent Serial Number The serial number of the parent serialized item. Note To create a change in the physical breakdown, the serialized item Status in the Serialized Items (tscfg2100m000) session must not be set to: Startup To be Recycled Superseded Removed You can use a dummy serial number for a Parent Item if the Dummy Serial Number check box is selected in the Serialized Items (tscfg2100m000) session. Change Number The number that identifies a change in the physical breakdown structure of the Parent Item. Note This value is defaulted from the Configuration Management Parameters (tscfg0100m000) session. Status The physical breakdown change status of the Parent Item. Allowed values Change Header Status Order Type The type of order that initiates the change in the physical breakdown structure of the Parent Item. Allowed values Order origin Note You can modify this value in the Physical Breakdown - Changes (tscfg2640m000) session only if the change Status is set to Free. This field is set to Maintenance Sales Order or Work Order only if the Depot Repair check box is selected in the General Service Parameters (tsmdm0100m000) session. This field is set to Service Order only if the Field Service check box is selected in the General Service Parameters (tsmdm0100m000) session. Order Number The code of the order that initiates the change in the physical breakdown structure of the Parent Item. Note You can modify this value in the Physical Breakdown - Changes (tscfg2640m000) session only if the change Status is set to Free. This field is applicable and mandatory only if the Order Type is set to: Maintenance Sales Order Work Order Service Order The order number must exist for the specified Order Type. Description The description or name of the Order Type/ Order Number. Note The value in this field is defaulted with the description of the order, when Order Type/ Order Number are specified. Created By The login code of the user who created the change. Note Default value is the login code of the user. Creation Date The date and time when the change is created. Note Default value is the system date and time. Item Superseded If this check box is selected, Infor LN indicates that the Parent Item and Parent Serial Number are superseded by the New Item and New Serial Number. New Item The code of the new item that supersedes the Parent Item. Note This item must be specified in the Item field and the Configuration Controlled field must be set to Serialized in the Items - Service (tsmdm2100m000) session. New Serial Number The serial number of the New Item that supersedes the Parent Item. Note To create a change in the physical breakdown structure, the serialized item Status in the Serialized Items (tscfg2100m000) session must not be set to: Startup To be Recycled Superseded Removed A physical breakdown structure must not exist for this item. You must not use a serialized item that supersedes another serialized item. Warehouse Order The code of the transfer order based on which the serialized item is superseded. When a serialized item that is present in the inventory is superseded, a transfer order is generated, which results in the change of Status the serialized item. Order Release only after Approval of Breakdown Changes If this check box is selected, ERP LN indicates that the status of the physical breakdown change must be approved in the Physical Breakdown - Changes (tscfg2640m000) session to process the linked order. Note This field is applicable only if the Order Number is specified. This field is disabled if the change Status is set to a value other than Free. |