| # Storage Inspections (qmptc2120m000) Use this session to maintain storage inspection orders which were generated in the Generate Storage Inspections (qmptc2220m000) session. You can also manually add new inspections. Related topics Storage inspections Item In LN, the raw materials, subassemblies, finished products, and tools that can be purchased, stored, manufactured, sold, and so on. An item can also represent a set of items handled as one kit, or exist in multiple product variants. You can also define nonphysical items, which are not held in inventory but can be used to post costs or to invoice services to customers. The following are examples of nonphysical items: Cost items (for example, electricity) Service items Subcontracting services List items (menus/options) Sequence The sequence number of the inspection order on the basis of which characteristics are tested on different samples. The default number is the highest number incremented by 1. Effectivity Unit The code that is linked to an end item for identification, and which can represent the deviation(s) from the standard end item. You can link an effectivity unit to manufactured items and purchased items. Note LN allows you to define sampling rules and testing combinations for specified Effectivity Unit. Related topics Effectivity units Inspection Quantity Ordered The quantity to be produced in a production order. The quantity you must inspect. It is the total of all the order quantities which are taken for storage inspection. Quantity Unit The physical quantity in which an item or good is managed. For example, a quantity of wood can be expressed as a length by using the unit of one meter, or as a volume by using the unit of one cubic meter. Status The inspection status indicates the current status of the inspection order. The status is changed during several sessions. Reason for Rejection The reason why the quantity is rejected. Accepted Quantities Recommended Quantity Accepted The quantity to be accepted, as recommended by the Quality package, expressed in the inventory unit. The total of all sample quantities which passed the tests successfully. Rejected Quantities Recommended Quantity Rejected The quantity to be rejected as recommended by the Quality package, expressed in the order unit. The total of all sample quantities which do not have the required quality level. Destroyed Quantities Quantity Destroyed The total quantity destroyed during a destructive test, expressed in the order unit. The quantity destroyed is equal to the sample size of the inspection orders that are tested by means of destructive tests. The quantity destroyed does not have any impact on the accepted or rejected quantities. LN only calculates the quantity that is destroyed according to the test. Dates Processing Date The date on which the inspection order lines are processed. |