| # Close Orders Inspection(qmptc1205m000) Use this session to check a range of origin orders (purchase, sales, or production orders) which have status Processed, and where the blocking method is Continue. LN checks which quantities are reported in the origin orders and compares them against the quantities which are entered in the Quality package. The results are displayed in a report. Related topics Order inspections Selection Range Origin An integrated module or package to which an (inspection) order is related. Origin Order The order number of the origin of the inspection. Origin Order Line The position number on the order to which the inspection order is linked. This can be the position number of the sales order line, the position number of the purchase order line, or the position number in the BOM. Operation One of a series of steps in a routing that are carried out successively to produce an item. The following data is collected during a routing operation: The task. For example, sawing. The machine used to carry out the task (optional). For example, sawing machine. The place where the task is carried out (work center). For example, woodwork. The number of employees required to carry out the task. This data is used to compute order lead times, to plan production orders and to calculate cost prices. Origin Order Sequence The sequence number of the inspection order on the basis of which characteristics are tested on different samples. Inspection Displays a list of the inspection order lines generated for a particular inspection order. These lines will correspond to characteristics maintained for each of the test groups that are linked to the Quality ID. Inspection Displays the sequence of the inspection that is carried out. Inspection Line An inbound advice or outbound advice number. Handling Unit A handling unit is a structure of packaging materials, or a part of such structure, used to pack items. A handling unit includes these attributes: Identification Code Packaging item (optional) Quantity of packaging items (optional) Important! If you link an item to a handling unit, the item is packed by means of the handling unit. The packaging item refers to the type of container or other packing material of which the handling unit consists. For Example: By defining a packaging item such as wooden crate for a handling unit, you specify that the handling unit is a wooden crate. Print Report If this check box is selected, LN prints the process report. Print Serials If this check box is selected, LN prints the serial numbers of the standard inspection order. Process Collectively checks and, optionally, closes the inspection orders for which you entered the test data. You can complete inspection orders by: Standard: Inspection orders are selected by origin as specified in the Testing Combinations session. Storage: A group of orders for storage inspection is selected. Order: A group of orders is selected based on their order number, without taking the origin into account. Before the inspection orders are completed, LN will check: whether or not the number of samples which have been taken for each inspection order is sufficient whether or not the number of inspection for each inspection order line is sufficient After the inspection order line has been completed, the status changes to Completed. As soon as all inspection order lines have order status Completed, the entire order is set to Completed. After an order line has been completed, it is not possible to add, modify, or delete any inspection data. |