| # Blocked Handling Units (whwmd6140m000) Use this session to to block or unblock handling units. Note You can view the peg distribution details for the blocked handling units using the Blocked Handling Units Details (whwmd6148m000) session. This session can be accessed using the Blocking Details option from the appropriate menu. Related topics To block and unblock Manual blocking of pegs Handling Unit The handling unit number that is used to uniquely identify the handling unit in LN. Status The handling unit's status. Handling Unit Status Reason for Blocking The reason code (of type Inventory Blocking excluding EP or Inventory Blocking including EP) as defined in the Reasons (tcmcs0105m000) session. Related topics Inventory blocking including or excluding EP User The logon code of the employee who activates a blocking. Only the user who activated a block can remove it Blocking Date The date and time of the blocking action. Warehouse A place for storing goods. For each warehouse, you can enter address data and data relating to its type. Location A distinct place in a warehouse where goods are stored. A warehouse can be divided into locations to manage the available space, and to locate the stored goods. Storage conditions and blocks can be applied to individual locations. Item In LN, the raw materials, subassemblies, finished products, and tools that can be purchased, stored, manufactured, sold, and so on. An item can also represent a set of items handled as one kit, or exist in multiple product variants. You can also define nonphysical items, which are not held in inventory but can be used to post costs or to invoice services to customers. The following are examples of nonphysical items: Cost items (for example, electricity) Service items Subcontracting services List items (menus/options) Lot A number of items produced and stored together that are identified by a (lot) code. Lots identify goods. Inventory Date The inventory date Text If this check box is selected, additional text related to the reason for blocking can be specified. |