| # Subassemblies Differences Infor LN 10.2.1 In Infor LN 10.2.1, a follow-up work order is created when a subassembly is processed using the Create Follow-up Order option from the action menu in the Work Order Material Resources (tswcs4110m000) session. New in Infor LN 10.3 In Infor LN 10.3, the outgoing subassembly is created manually from the Work Orders (tswcs2100m000) and Work Order (tswcs2100m100) sessions. The Create Follow-up Order option is no longer available. For more information, refer to Actions Performed on Incoming Subassemblies, Actions Performed on Outgoing Subassemblies and Processing Subassembly. |