| # Displaying Engineering BOM Note The following items can only be non-configurable items: Main item Sub item For more information on procuring purchased configurable items, refer to: Procuring configured items in Assembly Control - Master Data Setup Procuring configured items in Assembly Control - BOM setup Product variants - Purchased configurable items On the appropriate menu, you can: Edit the text of the parent revision. Start the Where Used EBOM Component (tiedm1550m000) session. Start the Exceptions (tcuef0105m000) session. Start the Reference Designators by Engineering Bom (tiedm2110m000) session. Edit the text of the selected component. Unit effectivity You can use effectivity units to model variations in the main item of the EBOM. You do not have to define a completely new EBOM for a variation for a particular customer. Instead, you define a standard configuration, and use exceptions to model the differences from the standard configuration. You can start the Exceptions (tcuef0105m000) session from the appropriate menu of this session. For more details about unit effectivity in EDM, click Unit effectivity in EDM. For more details about unit effectivity in LN in general, click Overview of unit effectivity. Related topics Engineering BOMs Engineering items Unit effectivity in EDM Overview of reference designators Defining alternative materials |