| # Test Group Characteristics (qmptc0137m000) Use this session to find, list and maintain groups of characteristics which are inspected in the same sample for a specific quality id. When inspection orders are generated, LN will generate: An inspection order for each test group. An inspection order line for each characteristic. All characteristics by test group are tested on the same sample. Note Before you can link groups of characteristics to a test group, you must define test groups in the Test Groups (qmptc0136m000) session, and the characteristics in the Standard Test Procedure Characteristics (qmptc0115m000) session. Related topics Standard test procedure and testing combinations Standard Test Procedure The code to which data is linked that is necessary to check the quality requirements of an item. Since one standard test procedure can be used for a group of products that require the same quality standards and tests, a standard test procedure can considerably reduce time. Test Group The definition of how often you take samples to test an order quantity, and what the sample size is. Aspect A part of an item. For example, a bolt can have the aspects head and tail. An aspect can have one or more characteristics. For example, a head can have a diameter and a length, and a tail can have a diameter and a color. Characteristic A reference to a particular quality or distinctive mark of an item or an item part/component. For example, diameter, length, weight. Test Sequence A number in this field specifies the sequence in which the characteristics are tested. By this you can sequence a characteristic with a destructive test as the last characteristic to be tested on the test quantity. |