| # Where-Used Standard Test Procedures (qmptc0116m000) Use this session to trace quality ID's. Standard Test Procedure The code of the standard test procedure that must be maintained. Description The description or name of the code. Combination Settings Origin An integrated module or package to which an (inspection) order is related. Quality Group The quality group, and all the items in it, for which a certain quality inspection is desired. Business Partner buy-from business partner/ sold-to business partner Note If you enter Purchase in the Origin field, you must enter a buy-from business partner in this field. If you entered Sales in the Origin field, you must enter a sold-to bussiness partner in this field. Item In LN, the raw materials, subassemblies, finished products, and tools that can be purchased, stored, manufactured, sold, and so on. An item can also represent a set of items handled as one kit, or exist in multiple product variants. You can also define nonphysical items, which are not held in inventory but can be used to post costs or to invoice services to customers. The following are examples of nonphysical items: Cost items (for example, electricity) Service items Subcontracting services List items (menus/options) E-Item Revision The version or revised version of an engineering item (E-item) or a revision-controlled item. Several revisions of an E-item can exist. Note Note: LN allows you to define sampling rules and testing combinations for specified E-Item Revision. Related topics Engineering Item Revision Description The description or name of the code. Effectivity Unit The code that is linked to an end item for identification, and which can represent the deviation(s) from the standard end item. You can link an effectivity unit to manufactured items and purchased items. Note LN allows you to define sampling rules and testing combinations for specified Effectivity Unit. Related topics Effectivity units Description The description or name of the code. Routing The sequence of operations required to manufacture an item. For each operation, the task, machine, and work center are specified, as well as information about setup time and cycle time. Operation The operation of the routing. During or after this operation, a certain quality inspection must take place. Task The task which is executed during the operation. From Warehouse The warehouse from which the item is transferred. Description The description or name of the code. Inspection Settings QM Only Recommends This field is used to indicate what can be done with the inspection results. If this check box is selected, the inspection results are a recommendation for the user; the user can overwrite these results. If this check box is cleared, the inspection results are mandatory; the user cannot overwrite these results. In this case you cannot use destructive tests. Note This field overrules the value of the QM Only Recommends field in the Quality Management Parameters (qmptc0100m000) session. Blocking Method for Inspections The blocking method refers to the way in which production, purchase, or sales is stopped or controlled to do inspections. Note If the QM Only Recommends check box is cleared, this field cannot be used. Text Displays text related to quality combinations. BOM Position The position in the BOM at which point a certain quality inspection is to take place. |