| # EBOM Copy Data (tiedm1120m000) Use this session to generate and maintain the copy data for a single-level engineering BOM. You can alter the details of the data of a particular line in the EBOM Copy Data (tiedm1120m000) details session. You can also use this session to change data generated by the Generate EBOM Copy Data (Multilevel) (tiedm1230m000) session and the Generate EBOM Copy Data by MBC (tiedm3235m000) session. Related topics Engineering data management summary Engineering BOMs Copying E-items to items Overview of reference designators Procedure for linking reference designators in the EBOM Reference designators and MBCs Defining alternative materials Engineering Item Enter the single-level EBOM's parent E-item that you want to copy. E-Item Revision Enter the parent E-item revision of the single-level EBOM that you want to copy. E-Item Revision The description or name of the code. Main Item Enter the parent item of the target production BOM (that is, the BOM to which you want to copy the single-level EBOM). Position Number The target position number of the PBOM line. Component Type Defines whether the component is an E-Item or Item. Component The source component in the EBOM line. EBOM Copy Method The copy method used by LN for copying the EBOM to the production BOM. Allowed values No Copy Action Copy E-Item to Item NonProj Item to Proj Item EBOM to Shop Floor PBOM Only EBOM copy method Related topics Engineering BOMs Finalized to Position The line number of the target production BOM, that is, the BOM to which you want to copy the data. Sequence Number The sequence number of the target BOM. Item Category The item category of the target item. To Item The target component item in the PBOM, which is the BOM line to which you want to copy the EBOM line. Related topics Engineering BOMs Copying E-items to items E-BOM Text If this check box is selected, a text is present. Length The length of the component in the EBOM line. Note Length can also be used to calculate Net Quantity:
    Net Quantity =
    			 Length x
    			 Width x
    			 Number of Units.
Width The width of the component in the EBOM line. Note Width can also be used to calculate Net Quantity:
    Net Quantity =
    			 Length x
    			 Width x
    			 Number of Units.
Number of Units The number of times the component occurs in the length (or area). For a physical item, this is equal to the number of units in the length or area defined. It can also be used to calculate Net Quantity:
    Net Quantity =
    			 Length x
    			 Width x
    			 Number of Units.
Net Quantity The net quantity of the component in the EBOM line. This is the amount of the component item used in the E-item. This can be calculated by multiplying the Number of Units, Length, and Width. Example: If ten units of a component 2 cm long and 3 cm wide are specified, the net quantity is calculated as 60. If the width is not specified, the net quantity is 20. Note You cannot define negative net quantities in the Engineering Data Management module. Related topics Scrap and yield Extra Information From the Extra Information field in the Engineering BOM (tiedm1110m000) session. You can use this field to enter a short note about the item or the BOM line. Description The description or name of the code. E-Item Copied If this check box is selected, then the E-item has already been copied to an item. E-Item Copied The date on which the E-item was copied to an item. EBOM Copied If this check box is selected, the single-level EBOM has already been copied to a production BOM. EBOM Copied The date on which the EBOM was copied to a PBOM. Description The name of the parent E-item revision of the single-level EBOM that you want to copy. Quantity Independent If this check box is selected, the E-item's net quantity is copied to update the scrap quantity in the BOM. If this check box is cleared, the E-item's net quantity is copied to update the net quantity of the BOM. Generate EBOM Copy data Click to generate EBOM copy data for the selection you have made in this session. If you want to generate copy data for the entire BOM, use the Generate EBOM Copy Data (Multilevel) (tiedm1230m000) session. Finalize Click to copy the data you have defined in this session. Use Up and Alternative Materials in EBOM Copy Data Click to start the Use Up and Alternative Materials in EBOM Copy Data (tiedm2125m000) session. |