| # Routing The planning data for the method of manufacturing is defined in Routing. A routing consists of operations, with each operation identifying the last to be carried out in a work center and/or on a certain machine. Routings can be as follows: Standard routing A generic routing that can be attached to multiple items Item specific A routing that is applied to one item Network routing A routing containing sequentially ordered operations and parallel operations Order quantity dependent routing A routing that is defined for a specific quantity of items You use the Routing module to record routings for manufactured items. You can define the following: Work centers A work center is where production activities are performed. Resources, such as people and machines, are lined to a work center. A work center is a group of resource units used as a functional planning unit. The operation rate code, which is linked to the work center, is used to calculate the cost price of an item or the estimated and actual costs. The capacity load on a work center is used in the planning of production. Work centers can be part of enterprise units used for multisite modeling purposes. Machines Machines are linked to work centers and are used to plan operations. The rate defined for a machine is used to calculate the actual machine costs. The capacity load on a machine is used for production planning. Tasks Classified according to the nature of the work performed, tasks are used to describe activities that take place on the shop floor. Tasks are linked to operation rate codes, which are used to calculate the cost price of an item or the estimated and actual costs. Tasks are used in production planning. Operations The operation data for standard and customized manufactured items is maintained with operations. Operation data is stored and maintained for standard items and customized items. A series of operations is performed to manufacture an item. The sequence of operations is defined as a routing in operations. Yield and scrap is defined per operation. Norm times The run time and production rate of an operation are determined using norm tables. After a matrix is defined for two physical characteristics, such as length and width you can maintain a set of standard operation times for the X-Y coordinates. When tasks and routings are defined, the run time and production rate can be calculated by using a norm table. |