| # Print Inspection Order Samples (qmptc1410m000) Use this session to print a range of samples. Related topics Order inspections Selection Range From Item Displays the From and To range of the From Item. This selection specifies the beginning of the range. To Item Displays the From and To range of the To Item. This selection specifies the end of the range. Origin Order Sequence Displays the From and To range of the sequence. Sequence The sequence number of the inspection order on the basis of which characteristics are tested on different samples. Origin An integrated module or package to which an (inspection) order is related. Origin Order The order number of the origin of the inspection. Origin Order The order number of the origin of the inspection. Origin Order Line The position number on the order to which the inspection order is linked. This can be the position number of the sales order line, the position number of the purchase order line, or the position number in the BOM. Position The position number on the order to which the inspection order is linked. This can be the position number of the sales order line, the position number of the purchase order line, or the position number in the BOM. Operation One of a series of steps in a routing that are carried out successively to produce an item. The following data is collected during a routing operation: The task. For example, sawing. The machine used to carry out the task (optional). For example, sawing machine. The place where the task is carried out (work center). For example, woodwork. The number of employees required to carry out the task. This data is used to compute order lead times, to plan production orders and to calculate cost prices. Operation One of a series of steps in a routing that are carried out successively to produce an item. The following data is collected during a routing operation: The task. For example, sawing. The machine used to carry out the task (optional). For example, sawing machine. The place where the task is carried out (work center). For example, woodwork. The number of employees required to carry out the task. This data is used to compute order lead times, to plan production orders and to calculate cost prices. Inspection Displays a list of the inspection order lines generated for a particular inspection order. These lines will correspond to characteristics maintained for each of the test groups that are linked to the Quality ID. Inspection Displays the sequence of the inspection that is carried out. Inspection Sequence An inbound advice or outbound advice number. Approval Number An inbound advice or outbound advice number. Handling Unit It is a structure of packaging materials, or a part of such structure, used to pack items. Handling Unit A handling unit includes the following attributes: 1)Identification Code. 2)Packaging item(optional). 3)Quantity of packaging items (optional). Important! If you link an item to a handling unit, the item is packed by means of the handling unit. The packaging item refers to the type of container or other packing material of which the handling unit consists. For Example: By defining a packaging item such as wooden crate for a handling unit, you specify that the handling unit is a wooden crate. Inspection Order An order used to structure the inspection of products that are purchased, produced, or sold. Inspection Order An order used to structure the inspection of products that are purchased, produced, or sold. Sample A small quantity that is drawn from the total (order) quantity and which represents the order quantity's quality. Sample A small quantity that is drawn from the total (order) quantity and which represents the order quantity's quality. Sampling Iteration The From and To fields define a range of: the sampling iterations. Print Displays the print option. Click Print to print all the samples in the range. |