| Overview of material issue |  |
| If you work on a production order, several methods are available to receive material on the shop floor. Backflushing The automatic issue of materials from inventory, or accounting for the hours spent manufacturing an item, based on theoretical usage and the quantity of the item reported as complete. For more information, refer to Backflushing. Floor stock A stock of inexpensive material present on the shop floor that can be used in production without recording each issue of material individually. Floor stock is not backflushed and is not part of the estimated costs. To account for floor stock materials, a surcharge is added to the cost price of an end item. A Kanban triggers the supply of floor-stock items to the shop floor. You can create a warehousing order of type SFC Production in which you determine from which warehouse and to what work center the material must be shipped. Controlled material issue Material is issued from the warehouse to the shop floor in a user-defined way. You can choose to take tight control over the issue process, or you can choose to control the issue process more loosely. In general, the issue of material goes through the following stages: Allocate material in the warehouse A planned production order results in planned inventory transactions. These transactions are used for planning purposes by the MRP planning engine. As soon as a production order is released, warehouse orders are created, which means that the material in the warehouse is allocated for the production order. All materials specified in the bill of material (BOM) are allocated in the warehouses, which is reflected in the Estimated Materials (ticst0101m000) session. If you use shop floor warehouses, you can determine the moment that the material is allocated in the shop floor warehouse. For more information, refer to Using shop floor warehouses. Specify quantity to be issued You must specify the material quantity that you want to issue. Depending on the setting of the Manual Issuing check box in the Shop Floor Control Parameters (tisfc0100s000) session, ERP LN automatically specifies the planned quantity, or you can manually specify the material quantity. Note that the material quantity is still blocked in the warehouse. For more information, refer to Specify material to be issued. Release material If you release the material in the warehouse, the material becomes unblocked, which is a signal for the warehouse employees to start the warehouse outbound procedure. For more information, refer to Release material. Carry out the warehousing procedure A user-defined warehouse outbound procedure is carried out. For more information, refer to Process warehouse order lines. Receive material The desired material quantity is received on the shop floor. To handle material from the warehouse to the shop floor, and from the shop floor to the warehouse, you can use the Material to Issue for Production Orders (ticst0101m100) session. To handle material in a more detailed way, you must use the Production Warehouse Orders (timfc0101m000) session. Particularly in case of serialized items or lot-controlled items, it is recommended that you use this session. All actions on material are laid out in so-called production warehouse orders, which you can view in the Production Warehouse Orders (timfc0101m000) session. Related topics Specify material to be issued Release material Process warehouse order lines Material issue parameters Backflushing Using shop floor warehouses Integrations of SFC with warehousing Direct processing of material shortages Labels in Manufacturing |