| Generate Maintenance Plan (tsspc2200m000) |  |
| Use this session to generate maintenance plans for a range of clusters. Note The start date for the serialized items is equal to the effective date of the serialized item (tscfg2100m000) session. The effective date is the installation time of the serialized item and if it is not filled then it is the delivery time and if the delivery time is also not filled then it is creation time of the serialized item. The serialized item's start value is equal to the planned dependent value that you defined for the serialized item in the Planned Activities (tsspc2100m000) session. Related topics Maintenance concept, prediction, and planning To specify a range To use From and To fields
Fields | Description
Cluster | The From and To fields define a range of: clusters.
Cluster | The From and To fields define a range of: clusters.
Sold-to BP | The From and To fields define a range of: sold - to business partners.
Sold-to BP | The From and To fields define a range of: the sold - to business partners.
Service Department | The From and To fields define a range of: service departments that execute the planned activity.
Service Department | The From and To fields define a range of: service departments that execute the planned activity.
Work Center | The From and To fields define a range of: the work centers that executes the planned activity.
Work Center | The From and To fields define a range of: the work centers that execute the planned activity.
Serialized Item Group | The From and To fields define a range of: serialized item groups s.
Serialized Item Group | The From and To fields define a range of: the serialized Item groups.
From Item | The From and To fields define a range of: the items.
From Serial Number | The From and To fields define a range of: serial numbers
To Item | The From and To fields define a range of: the items.
To Serial Number | The From and To fields define a range of: serial numbers
Include Independent Serials |
Generate Including Child Items. | If this check box is selected, the planned activities for the child items are generated for a serialized item or a cluster configuration line.
Time | Activities will only be planned for the clusters during the time range you specify. This is the start value of your time range.
Time | Activities will only be planned for the clusters during the time range you specify. This is the end value of your time range.
Method | Determines when the maintenance cycle starts.
Consider Last Planned Activity Date |
Activity Status | The status of the activities being generated for the maintenance plan. The activity status can either be Free, Released or Final.
Process Report | Process report
Error Report | Error report