| Sample Test Data by Characteristic History (qmptc3515m000) |  |
| Use this session to display the test data history by characteristic. The data was previously entered in the Sample Test Data by Characteristic (qmptc1115m000) details session. Test data lines were generated based on the test quantity (see the Inspection Order Samples (qmptc1110m000) session). Example
Sample quantity | 100 pieces
Test quantity | 20 pieces
Explanation: You need to do five tests on twenty pieces to get a sample quantity of one hundred pieces (100/20=5). Consequently, five test lines are generated. Related topics Standard inspections
Fields | Description
Inspection Order | The code of the inspection order.
Sample | A small quantity that is drawn from the total (order) quantity and which represents the order quantity's quality.
Aspect | A part of an item. For example, a bolt can have the aspects head and tail. An aspect can have one or more characteristics. For example, a head can have a diameter and a length, and a tail can have a diameter and a color.
Position | The position number represents a characteristic that is measured. The measured value is entered as test data in the Sample Test Data by Characteristic (qmptc1115m000) session, or the Sample Test Data by Serial Number (qmptc1116m000) session.
Characteristic | A reference to a particular quality or distinctive mark of an item or an item part/component. For example, diameter, length, weight.
Serial Number | A unique number generated by ERP LN to distinguish between the different measurements you can do in one sample quantity. The number of measurements is based on the test quantity.
Example
Sample quantity | 100 pieces
Test quantity | 20 pieces
Explanation: You need to do five tests on twenty pieces to get a sample quantity of one hundred pieces (100/20=5). Consequently, five test lines are generated, with each an unique serial number. Note The total number of serial numbers cannot exceed the value of the sample quantity divided by the test quantity
Characteristic Type | The type of value that is measured.
Item | In ERP LN, the raw materials, subassemblies, finished products, and tools that can be purchased, stored, manufactured, sold, and so on. An item can also represent a set of items handled as one (kit), or exist in multiple product variants (generic item). You can also define nonphysical items, which are not held in inventory but can be used to post costs or to invoice services to customers. Examples of nonphysical items: Cost items (for example, electricity) Service items Subcontracting items List items (menus/options)
Test Date | The date and time when the test took place.
Measurement Value | The result of the test. A numeric value is displayed if you selected Quantitative in the Result Type field, and if the Characteristic Type field was not set to Option. If an algorithm was specified for the inspection order line, the algorithm calculated the numeric value that is displayed in this field.
Frequency Unit | The unit in which the test results are defined or calculated. Note This field does not apply if you entered Option in the Characteristic Type field.
Option Set | The name of the option set.
Option | The option that was found. Note Depending on what you entered in the Option Type field in the Options (qmptc0114m000) session, the option is either Acceptable or Not Acceptable.
Test Area | The physical location where tests take place.
Employee | The person that performs the test on this characteristic.
Instrument | The default instrument used to measure the characteristic.
Result | The result of the inspection. Note ERP LN automatically generates a value, depending on the quality limits that you defined in the Quality ID - Characteristics (qmptc0115m000) session and/or in the Options (qmptc0114m000) session.