| Finalize Engineering Data (tiedm3240m000) |  |
| Use this session to finalize copying data from EBOMs to PBOMs, that is, to actually copy the data which you have generated in previous sessions. Update methods You can either finalize data using mass bill of material changes (MBCs), or you can finalize data for individual items. Before you run this session for individual E-items, you must record the EBOM copy data for those items in the EBOM Copy Data (tiedm1120m000) session. Before you run this session for revisions generated by MBC, you must run the Generate EBOM Copy Data by MBC (tiedm3235m000) session. Selection range If you select With MBC in the Finalization Method field you can select the range of MBCs for which you want to finalize data. If you select Without MBC in the Finalization Method field: you can select the range of E-item revisions and main items (parent BOM items) for which you want to finalize data. Note The MBC cannot be finalized if E-items have been recorded using MBCs, but these E-items have no relationship with an item. Related topics Finalizing engineering data Engineering data management summary Copying E-items to items Engineering BOMs To change EBOMs - Automatic procedure
Fields | Description
Finalization Method | Use this session to finalize copying data from EBOMs to PBOMs. Update Methods You can either finalize data using MBCs or finalize data for individual items. You can also select whether all BOM lines are copied, or only certain ones. Selection Range If you have selected With MBC in the Finalization Method field, you can select the range of MBCs for which you want to finalize data. If you have selected Without MBC in the Finalization Method field, you can select the range of E-item revisions and Main items (parent BOM items) for which you want to finalize data. Related topics Engineering data management summary Finalizing engineering data Engineering BOMs
Production BOM Update Method | Select the method by which you want to copy data from the engineering BOM (EBOM) to the production BOM. If the PBOM History check box in the Engineering Data Management Parameters (tiedm0100m000) session is cleared, the production BOM lines are overwritten by the copied data. If that check box is selected, the copied data is written to new sequence numbers. Allowed values Possible values Related topics Engineering BOMs Finalizing engineering data To use From and To fields
MBC Number | Select the range of MBCs which you want to use to copy data from engineering to production.
MBC Number | Select the range of MBCs which you want to use to copy data from engineering to production.
From Engineering Item | Select the range of E-items whose revisions you want to copy from engineering to production. If the copy data you have generated includes the bills of material for these items, they will be copied as well.
To Engineering Item | Select the range of E-items whose revisions you want to copy from engineering to production. If the copy data you have generated includes the bills of material for these items, they will be copied as well.
Engineering Item Revision | Select the range of E-item revisions you want to copy from engineering to production. If the copy data you have generated includes the bills of material for these items, they will be copied as well.
Revision | Select the range of E-item revisions you want to copy from engineering to production. If the copy data you have generated includes the bills of material for these items, they will be copied as well.
From Main item | Select the range of target production items you require. The result of copying an E-item to this item depends on the value of the item's Update Engineering Item Relations field in the Items - General (tcibd0501m000) session. You can alter the Update Engineering Item Relations field with the Update Engineering Relationship (tiedm3220m000) session.
To Main item | Select the range of target production items you require. The result of copying an E-item to this item depends on the value of the item's Update Engineering Item Relations field in the Items - General (tcibd0501m000) session. You can alter the Update Engineering Item Relations field with the Update Engineering Relationship (tiedm3220m000) session.
Finalize Multilevel | If this check box is selected, the data is finalized on multilevel, instead of at single-level. For example, if you have an EBOM structure of A-B-C and you perform multilevel finalizing, when you finalize A, the EBOMs of B and C are also finalized.
Copy Document Links | If this check box is selected, all attached documents are also copied during the copy process. For example, if you have an EBOM structure of A-B-C and you perform multilevel finalizing, when you finalize A, the attached documents of B and C are also finalized.
Overwrite existing PBOM | If this check box is selected, an existing PBOM is overwritten without creating a new revision for the top E-item. You can select this check box if many sub-level changes must be finalized, and it is not desired to create a new revision for the top E-item. The error message Valid E-BOM copy data not present is suppressed, and further action is continued in the session.