| Cluster - Lines (tsbsc1110m000) |  |
| Use this session to maintain configurations for a selected cluster. Example Two engines, each of which has the code CF6, and which belong to your business partner MACH Industries (MACHI), are identified as one cluster. The cluster is called CF6 machine MACHI. Note You can use the Sort by command on the View menu to choose the way you want to display the cluster data. On the Specific menu, you can choose: Create Physical Breakdown- Enables you to generate a physical breakdown structure from one of the following: Item breakdown As-built structure ASCII file Project-breakdown structures Physical Breakdown- Enables you to view or maintain the multilevel or single-level parent-child relations between serialized items that form a physical breakdown. A physical breakdown is defined for a configuration, which enables you to view the configuration's built-up structure and as-maintained structure. Item Breakdown- Enables you to view or maintain the parent-child relations between items that form an item breakdown. Item Details- Starts the Serialized Items (tscfg2100m000) session. Activate Cluster Configurations- Starts the Activate Cluster Configurations (tscfg2210m500) session, which enables you to switch the status of multiple configurations to Active in one run.
Fields | Description
Cluster | The cluster to which the configurations, anonymous items. or serialized items are linked.
Description | The description or name of the cluster.
Line Number | The number that identifies an anonymous item or a serialized item in the cluster.
Item | The anonymous item that can belong to an item breakdown and that is linked to this cluster. The number in the Cluster Configuration Line field identifies the item (breakdown) for the cluster. Note For an anonymous item, you can specify a quantity in the Number of Items field. To link a serialized item to the cluster, you must select the item's serial number in the Serial Number field.
Serial Number | To link a serialized item to this cluster, you can enter the item's serial number in this field. Note This field is not available if you have entered a quantity for the anonymous item.
Description | The description or name of the item.
Number of Items | The number of anonymous items for this cluster configuration line. Note This field is not available if you link a serialized item to this cluster.
Status Start Time | The time when the Status field is set or changed.
Status | The Status of the cluster line.
Planned Until Time | The date and time until when the maintenance activities are planned for the cluster configuration. Note The date of the planned until time must fall within the effective period of this cluster configuration. This field is a display field.
Commands | Description
Create Physical Breakdown | Displays the various options to create a Physical Breakdown. The options available to create a Physical Breakdown are: From Item Breakdown. From As-built structure. From ASCII File. From Project Breakdown structure.
From Item Breakdown... | Use this option to create a physical breakdown from Item breakdown.
From As-built Structure... | Use this option to create a physical breakdown from As-Built Structure.
From ASCII-File... | Use this option to create a physical breakdown from ASCII file.
From Project Breakdown Structures... | Use this option to create a physical breakdown from Project Breakdown Structures.
Physical Breakdown | Starts the Physical Breakdowns (tscfg2110m000) session.
Item Breakdown | Starts the Item Breakdowns (tscfg1110m000) session.
Item Details | Starts the Serialized Items (tscfg2100m000) session.
Activate Cluster Configurations | Starts the Activate Cluster Configurations (tscfg2210m500) session.