| Inspections (tssoc2550m000) |  |
| Use this session to register the results of inspections on a serialized item, which are carried out as part of a service order activity. You register inspections based on the measurement that are listed for the reference activity's inspection template in the Reference Activity - Measurement Types (tsacm3160m000) session. This is typically used in a condition-based maintenance (CBM) regime, in which inspections are planned for, and carried out on, serialized items. Note You can only maintain inspection results for a service order, when the service order's status is Released or Completed. When you fill in all the inspection data, ERP LN immediately copies the inspection results to the Serialized Items Inspections History (tssoc2551m000) session. If you leave the Registration Time field, Dependent Value (Y-axis) field and the Independent Value (X-axis) field empty, ERP LN does not copy the inspection results to the Serialized Items Inspections History (tssoc2551m000) session. When you delete the inspection data from the Inspections (tssoc2550m000) session, ERP LN also removes the inspection data from the Serialized Items Inspections History (tssoc2551m000) session. You cannot start this session if the Use Measurements check box in the Service Planning and Concepts Parameters (tsspc0100m000) session is cleared. In this case, ERP LN displays the SPC parameter 'Use Measurements' not found! message when you try to start this session. Related topics To use an overview session To maintain records in an overview/maintain session
Fields | Description
Item | The item code of the serialized item, on which you carry out and register the inspections for.
Serial Number | The serial number of the item, on which you carry out and register the inspections for.
Service Order | The (code of the) service order that the inspections are carried out and registered as part of.
Activity Line Number | The activity line number in the service order, that the inspections are carried out for. Note You can only maintain this field when: The Service Order field is filled. The activity line entered is defined for the service order. In the Service Order Activities (tssoc2110m000) session the Cluster, Item, Serial Number, and Reference Activity fields are all filled.
Reference Activity | The code of the reference activity given to the inspections carried out. Note You use the reference activity's inspection template (defined for it in the Reference Activity - Measurement Types (tsacm3160m000) session) to register inspections in this session.
Measurement | The measurement that the inspection line uses. Note You can only select measurement listed for the reference activity's inspection template in the Reference Activity - Measurement Types (tsacm3160m000) session.
Sequence | The unique number given to an inspection line to distinguish it from the other inspections registered for the serialized item (as part of the service order activity).
Registration Time | The time at which you register the inspection for the serialized item. Default value The time at which you enter the inspection line in ERP LN. Note To register an inspection for a serialized item linked to: A cluster (in the Cluster - Lines (tsbsc1110m000) session), the registration time must fall between the cluster's effective time and expiry time. A top serialized item (in the Physical Breakdowns (tscfg2110m000) session), the registration time must fall between the effective time and expiry time of the top serialized item (component).
Dependent Value (Y-axis) | The value of the dependent variable when the inspection is carried out. Note If you leave this field empty, ERP LN does not copy the inspection results to the Serialized Items Inspections History (tssoc2551m000) session.
Dependent Value | The unit used to express the value of the measurement's dependent variable.
Independent Value (X-axis) | The value of the independent variable when the inspection is carried out.
Independent Value | The unit used to express the value of the measurement's independent variable.
Follow-up | If this check box is selected, a follow-up activity can be created for the inspection. If this check box is cleared, a follow-up activity cannot be created for the inspection.
Follow-up Activity | The follow-up activity that must be executed. This activity defaulted from the Inspection Template.
Reason | The reason code to execute the Follow-up activity.
Description | The description of the reason.
Follow-up Service Order/Activity | The number assigned to the newly created Follow-up Service Order or Activity.
Follow-Up Activity | The activity line number of the follow-up activity.
Activity Line | The description of the Follow-up Service Order/Activity.
Free Text | Text (additional)
Dependent Norm Value | The norm value of the dependent variable. It determines when maintenance is desirable for the Serialized Item.
Upper Limit Value | The maximum value of the dependent variable. The measurement must not exceed the upper limit value.
Lower Limit Value | The minimum value of the dependent variable. The measurement must not go below the lower limit value.
Out of Limit Warning | The warning given to the user when the measurement of the dependent variable is not within the stipulated range.
Commands | Description
Follow-up | Use this command to create a follow-up activity.
Create New Order and Activity | Use this command to create a new order or activity.
Create Activity under Current Order | Use this command to create an activity under the current order.
View Inspections(History) | Starts the Serialized Items Inspections History (tssoc2551m000) session.