| Line Segment - Stations (tiasl1550m000) |  |
| Use this session to display or modify the line stations of an assembly line segment and their relationship to each other. You can display the current effective stations or all the stations for a Line Segment. To edit the data, double-click a line, or click the New button. Assembly lines are composed of a series of segments. Segments are composed of a buffer and one or more line stations, until the next buffer. You can link line stations in the Work Centers (tirou0101m000) session. To define which line stations are linked to which segment, for a particular date, you can use the details session or the line definition procedure of Configurator. Specific menu You can use the Specific menu to start one of the following sessions: Line Station - Assembly Orders (tiasl6510m000) Buffer - Assembly Orders (tiasl6520m000) Assembly Line - Assignments and Line Stations (tiasc5520m000) On the Specific menu, you can also choose whether you want to view all stations, or the current effective stations only. Related topics Assembly control overview Line station variants
Fields | Description
Line Segment | A set of consecutive assembly-line work centers on an assembly line between two buffers. The first buffer is the beginning of the segment, the next buffer is the first part of the next segment.
Line Segment | A set of consecutive assembly-line work centers on an assembly line between two buffers. The first buffer is the beginning of the segment, the next buffer is the first part of the next segment.
Station | A line station or a line buffer that is linked to the line segment.
Station Type | The type of the line station.
Next Station | The station that comes after the station or buffer defined in the Station field.
Effective Date | The first date when the line stations in this line are valid. This field cannot be empty.
Expiry Date | The last date when the line stations in this line are valid. If this field is empty, the stations are always valid.