| # Generate Supply Orders for Subcontracting (tdpur4216m000) Use this session to generate supply orders or supply schedules by means of which materials are shipped from the manufacturer or from the manufacturer's supplier to the subcontractor for operation subcontracting, or item subcontracting. For each subcontracting purchase order, you can view which materials and subassemblies must be supplied to the subcontractor in the Purchase Order Material Supply Lines (tdpur4116m000) session. The materials can be supplied by means of a sales transfer order, sales transfer schedule, warehouse transfer, purchase supply order, or purchase supply schedule, which you define in the Purchase Order Material Supply Lines (tdpur4116m000) session. Transfer supply order/schedule If the Supply Type is set to Warehouse, you can define the type of transfer supply order that is generated in the Transfer Type field. Purchase supply order/schedule If the Supply Type is set to Supplier, the Purchase Schedule in Use check box in the Item - General (tcibd0101s000) session determines whether a purchase supply order, or a purchase supply schedule must be generated to order the material from the Buy-from Business Partner, who next delivers it to the subcontractor. Note You can view the number of the supply order or schedule that is generated to supply the materials in the Supply Order Number field of the Purchase Order Material Supply Lines (tdpur4116m000) session. You must only use this session in the purchase order procedure if the following two conditions are applicable: The Responsible for Supply Planning check box is selected in the Purchase Order Material Supply Lines (tdpur4116m000) session. If the Responsible for Supply Planning check box is cleared, the subcontractor is responsible for obtaining the required materials. The supply system is Order Controlled/Single, which you can define in the Warehouse - Item (whwmd2510m000) session. Related topics Overview of subcontracting Flexible purchase order processing Print Errors If this check box is selected, and errors occur during the generation process, an error report is printed. |