| # Print Physical Breakdowns (tscfg2410m000) Use this session to print the physical breakdown. Note LN only prints the serialized items that have the Active status on the date you enter in the Configuration as On field. Refer to the Physical Breakdown Log (tscfg2515m000) session, for changes to the physical breakdown. Use the graphical browser framework (GBF), to view the entire physical breakdown (including expired and future items). If you select the Display by Alternate Serial Numbers check box in the Configuration Management Parameters (tscfg0100m000) session, the serialized items are displayed by the business partner's serial number when you zoom in the Item fields. Cluster The start value in the range of clusters whose constituent item's physical breakdowns you wish to print. Cluster The end value in the range of clusters whose constituent item's physical breakdowns you wish to print. From Item The start value in the range of serialized items whose physical breakdowns you wish to print. To Item The end value in the range of serialized items whose physical breakdowns you wish to print. From Serial Number The start value in the range of serialized items whose physical breakdowns you wish to print. Note If you select the Display by Alternate Serial Numbers check box in the Configuration Management Parameters (tscfg0100m000) session, the serialized items are displayed by the business partner's serial number when you zoom in this field. To Serial Number The end value in the range of serialized items whose physical breakdowns you wish to print. Note If you select the Display by Alternate Serial Numbers check box in the Configuration Management Parameters (tscfg0100m000) session, the serialized items are displayed by the business partner's serial number when you zoom in this field. Print Current Configuration If this check box is selected, LN prints the current configuration. If this check box is cleared, you can specify a date before the current date in the Configuration as On field. Configuration as On LN prints the item's physical breakdowns as they were, or are, on the date you enter in this field. Note LN only prints the serialized items that have the Active status on this date. Refer to the Physical Breakdown Log (tscfg2515m000) session, for changes to the physical breakdown. Level Selects the level of items that you print. Sorted By Specify the sequence in which the selected data must be printed. Physical Breakdown Log If this check box is selected, LN prints the Physical Breakdown Log. |