| # Effective Assembly Line Surcharge Base (ticpr3160m000) Use this session to display the effective assembly line surcharge base for a specific assembly line. You can view the effective assembly line surcharge base in this session, after you actualized the assembly line surcharges in the Actualize Assembly Line Surcharges (ticpr2280m000) session. An assembly line surcharge base is a set of cost components based on which the assembly line surcharge must be calculated. You must use an assembly line surcharge base if the surcharge calculation method for the assembly line surcharge is Selective (Total Costs), or Selective (Added Costs). The surcharge calculation method is defined in the Assembly Line Surcharges (ticpr1180m000) details session. Related topics Cost components in Manufacturing Assembly order costing Assembly Line A set of consecutive line stations in which FAS (Final Assembly Schedule) items are manufactured. The items are manufactured by passing the items from line station to line station and by carrying out operations at each line station. An assembly line is subdivided into a number of line segments separated by buffers. An assembly line can be either a main line or a supplying line. Generic Item An item that exists in multiple product variants. Before any manufacturing activities are performed on a generic item, the item must be configured to determine the desired product variant. Example Generic item: electric drill Options: 3 power sources (batteries, 12 V or 220 V) 2 colors (blue, gray). A total of 6 product variants can be produced with these options. Effective Date The date and time on which the assembly line surcharges take effect. Sequence The sequence number of the assembly surcharge line. Cost Component The cost component to which the assembly line surcharge is linked. Related topics Cost components in Manufacturing |