| # Planned Activities - Cluster (tsspc2100m000) Use this session to view and maintain the list of activities planned for the preventive maintenance of a cluster. A list of activities can be generated for a cluster, or a range of clusters, using the Generate Maintenance Plan (tsspc2200m000) session. The generated planned activities for the cluster are based on the maintenance concepts of its constituent items. Planned activities can also be added manually using the details session. Cluster The code of the cluster for which the activities are planned. Cluster The name or description of the cluster. Activity The code of the planned activity. Activity This number distinguishes activities with the same reference code. Note The displayed reference activities are sorted into groups with the same reference code. The groups are listed in alphabetical order. The order within the groups is determined by the sequence number. When LN generates planned activities from a maintenance concept containing activities with identical codes, it gives higher sequence numbers to activities with later start times. This way the activities are displayed chronologically within their groups. When you manually add an activity, it is advisable to give a sequence number that will display your added activity in the correct chronological sequence for its group. Description The name or description of the planned activity. Search Argument An alternative form of a description used for convenience during searching. A search key is usually an abbreviation, an acronym, or a mnemonic alternative to a full description. Status Status of the planned activity. Allowed values Status Planned Activity Text Text (additional) Item The code of the item for which the activity is planned. Serial Number The serial number of the item for which the activity is planned. Alternate Serial Number If business partner's use their own serial numbers as an alternative to item's manufactured one, the business partner's alternative is given in this field. Note Alternate serial numbers are given in the Serialized Items (tscfg2100m000) session. Description The name or description of the item. Downtime Ratio The percentage of an activity's duration that an item will be out of operation when the activity is carried out on the item. The downtime ratio can be used for internal maintenance to determine the work-center capacity. For the percentage of the activity's duration, the capacity of the work center is reduced. Planned Finish Time Planned finish time of the activity. Earliest Start Time The activity's earliest acceptable start time. The default value is determined by the the reference activity's Tol. Period selected in the Reference Activities (tsspc1100m000) details session. Latest Finish Time The activity's latest acceptable finish time. The default value is determined by the the reference activity's Tol. Period selected in the Reference Activities (tsspc1100m000) details session. Appointment If this check box is selected, an appointment has been arranged with the customer for the planned activity to be carried out by the service engineer. If this check box is cleared, no appointment has been arranged. Measurement Type A particular measurement that is used to determine the value of an item's variable (measuring quantity) in a specific situation. Example: Tire tread depth. Measurement Type The name or description of the measurement type. Independent The value of the independent variable when the activity must be carried out. This is when the dependent variable is expected to reach its norm value. Independent The unit used to express the value of the independent variable. Dependent When the activity is planned to be carried out on the item, it is expected that the value of the dependent variable will have reached this value which, by default, is the dependent norm value of the measurement type. Dependent The unit used to express the value of the dependent variable. Service Department The service department that carries out the reference activity. Note The default value is that given to the activity in the Reference Activities (tsspc1100m000) details session. Service Department The name of the service department. Checklist Lists the points to which the service engineer must pay attention during the execution of a service activity. Checklists are used to group specific checks so that more than one check can be defined for a reference activity. According to the answers expected from the check, space is provided when printing the document related to the service order. Note The default value is that given to the activity in the Reference Activities (tsspc1100m000) details session. Checklist The description or name of the checklist. No. 1 The specific knowledge or technical expertise that a service engineer must have to carry out service or maintenance activities. For example, knowledge of electricity, specific equipment, and so on. Service skills can be used as constraints when planning orders. Note The default value is that given to the activity in the Reference Activities (tsspc1100m000) details session. No. 1 The description or name of the service skill. No. 2 The specific knowledge or technical expertise that a service engineer must have to carry out service or maintenance activities. For example, knowledge of electricity, specific equipment, and so on. Service skills can be used as constraints when planning orders. No. 3 The specific knowledge or technical expertise that a service engineer must have to carry out service or maintenance activities. For example, knowledge of electricity, specific equipment, and so on. Service skills can be used as constraints when planning orders. Service Order The number of the related service order if the maintenance plan was transferred to the Service Order Control module. Service Order The status of the related service order. Activity Line Number The number of the related service order activity line, if applicable. Planned Start Time Planned start time of the activity. Activity Duration The duration of the planned activity. The default value is that given to the activity in the Reference Activities (tsspc1100m000) session. Travel Duration The time required to travel from the service department to the cluster's location. The default value is that given to the cluster in the Clusters (tsbsc1100m000) session. Activity Group The code of the activity's activity group Buy-from B.P. The code of the buy-from business partner who carries out any subcontracted work required by the activity. Buy-from B.P. The name of the subcontractor. Service/Cost Item The code of the service item or cost item required in order to complete the reference activity if a subcontractor is required. The service/cost item is used on a purchase order line. The item is required because you cannot add an activity to a purchase order line, the item will be used as an activity definition. This item will be used as a default item when generating purchase orders. Description The name or description of the item. Activity Group The name or description of the activity group. Coverage Type A financial classification that indicates to what extent work is covered under warranty or contract, and what part of the activities can be charged. Coverage Type The name or description of the coverage type. Owner The sold-to business partner or the internal department that owns the cluster. |