| # Process Inspection Orders (qmptc1204m000) Use this session to process inspection orders with status Completed. The recommended accepted, rejected, and destroyed quantities are calculated. The steps in this process are as follows: LN selects all inspection orders for each origin with status Completed LN selects inspection orders by test type: Single sampling. 100% or continuous sampling. The samples are selected, for each inspection order. For each sample selected, LN determines the number of: Good pieces Bad pieces LN consolidates the inspection results for all the samples. LN calculates the actual acceptance percentage and compares the results with the Acceptable Quality Level field in the Test Groups (qmptc0136m000) session. If the Acceptable Quality Level is reached, the order quantity is accepted. After the inspection order has been processed, the order status changes to Processed. Tabs Standard Processes a range of inspection orders, selected by origin. Storage Processes a range inspection orders, selected by item. Related topics Standard inspections Origin An integrated module or package to which an (inspection) order is related. Origin Order The order number of the origin of the inspection. Line The position number on the order to which the inspection order is linked. This can be the position number of the sales order line, the position number of the purchase order line, or the position number in the BOM. Operation One of a series of steps in a routing that are carried out successively to produce an item. The following data is collected during a routing operation: The task. For example, sawing. The machine used to carry out the task (optional). For example, sawing machine. The place where the task is carried out (work center). For example, woodwork. The number of employees required to carry out the task. This data is used to compute order lead times, to plan production orders and to calculate cost prices. Sequence The sequence number of the inspection order on the basis of which characteristics are tested on different samples. Inspection Displays a list of the inspection order lines generated for a particular inspection order. These lines will correspond to characteristics maintained for each of the test groups that are linked to the Quality ID. Inspection Displays the sequence of the inspection that is carried out. Approval Number An inbound advice or outbound advice number. Handling Unit A handling unit is a structure of packaging materials, or a part of such structure, used to pack items. A handling unit includes these attributes: Identification Code Packaging item (optional) Quantity of packaging items (optional) Important! If you link an item to a handling unit, the item is packed by means of the handling unit. The packaging item refers to the type of container or other packing material of which the handling unit consists. For Example: By defining a packaging item such as wooden crate for a handling unit, you specify that the handling unit is a wooden crate. From Item In LN, the raw materials, subassemblies, finished products, and tools that can be purchased, stored, manufactured, sold, and so on. An item can also represent a set of items handled as one (kit), or exist in multiple product variants (generic item). You can also define nonphysical items, which are not held in inventory but can be used to post costs or to invoice services to customers. Examples of nonphysical items: Cost items (for example, electricity) Service items Subcontracting services List items (menus/options) To Item In LN, the raw materials, subassemblies, finished products, and tools that can be purchased, stored, manufactured, sold, and so on. An item can also represent a set of items handled as one (kit), or exist in multiple product variants (generic item). You can also define nonphysical items, which are not held in inventory but can be used to post costs or to invoice services to customers. Examples of nonphysical items: Cost items (for example, electricity) Service items Subcontracting services List items (menus/options) Process Collectively processes the inspection orders for which you entered the test data. You can complete inspection orders by: Standard: Inspection orders are selected by origin as specified in the Quality Combinations (qmptc0111m000) session. Storage: A group of orders for storage inspection is selected. Order: A group of orders is selected based on their order number, without taking the origin into account. Before the inspection orders are completed, LN will check: whether or not the number of samples which have been taken for each inspection order is sufficient whether or not the number of inspection for each inspection order line is sufficient After the inspection order line has been completed, the status changes to Completed. As soon as all inspection order lines have order status Completed, the entire order is set to Completed. After an order line has been completed, it is not possible to add, modify, or delete any inspection data. |