| # Create Physical Breakdown Structure from ASCII-File (tscfg2210m100) Use this session to create a physical breakdown structure from an ASCII file that can be, for example, a parts list of an illustrated parts catalog in ASCII format. Note The items in the ASCII file must exist in the Items - General (tcibd0501m000) session, before you can create the physical breakdown from the ASCII file. If you run this session, LN automatically generates the items in the Items - Service (tsmdm2100m000) session and the serialized items in the Serialized Items (tscfg2100m000) session. You can create a new (unlinked) physical breakdown or you can link the newly-created physical breakdown to a cluster or to a serialized item (component) in an existing physical breakdown. Related topics To create a physical breakdown from an ASCII file Link To Select how the newly created physical breakdown must be linked. Allowed values Link to Cluster The cluster to which the physical breakdown must be linked. Note To enable this field, select the Cluster option in the Link To field. Cluster The description or name of the code. Item The serialized item of an existing physical breakdown to which the newly-created physical breakdown must be linked. Serial Number The serial number of the serialized item. Description The item's name or description. Serialized Item Group The serialized-item group of the newly-created serialized items. Note If the Serialized Item Group Usage parameter check box in the Configuration Management Parameters (tscfg0100m000) session is selected, this field must be filled. Serialized Item Group The name or description of the serialized item group. Delivery Time The delivery time of the serialized item. Input File The path where the ASCII file is located. Example: `/home/rkrishna/textfile.txt` Error Report Error report Process Report Process report |