| Serialized Items Inspections History (tssoc2551m000) |  |
| Use this session to view the results of inspections carried out on a serialized item. You can also search for the list of inspections that has been conducted on a serialized item based on the search criteria. After you enter relevant details in the To and From fields, click on the Apply button, relevant inspection details on the serialized items are listed. Note When all inspection data is filled in, ERP LN immediately copies the inspection results that you enter in the Inspections (tssoc2550m000) session to the Serialized Items Inspections History (tssoc2551m000) session. When you delete the inspection data from the Inspections (tssoc2550m000) session, ERP LN also removes the inspection data from the Serialized Items Inspections History (tssoc2551m000) session. If the Use Measurements check box in the Service Planning and Concepts Parameters (tsspc0100m000) session is cleared, you cannot use this session. ERP LN displays a message.
Fields | Description
Item | The item code of the serialized item, for which the inspections are registered. The code consists of a project code field and an item code field.
Serial Number | The serial number of the serialized item.
Measurement | The code of the measurement on which the inspection is based.
Seq. | This sequence number identifies a unique measurement for each item.
Registration Time | The time on which the measurement is carried out. This field indicates the registration time for the inspection. Note The field must be linked to a service order and it can be filled only when the activity line status is either released or completed.
Dependent Norm Value | The dependent norm value determines the moment that maintenance is required for the serialized item of the cluster.
Dependent Norm Value | The unit of the measuring quantity that is defined for the dependent variable of the measurement.
Dependent Value | A unit of measurement, which together with a norm value (and start value) determines when maintenance activities must be carried out.
Dependent Value | The unit of the measuring quantity that is defined for the dependent variable of the measurement.
Independent Value | In the case of counter values (CV) or predicted activities (PA), the measurement type's independent variable of a will be of type time. In case of predicted inspections (PI), it can also be usage related. Example A tire has two variables: the number of kilometers traveled, and the depth of its tread. Each kilometer traveled by the tire decreases its tread depth. In this case, the independent variable is the number of kilometers traveled by the tire, and is usage related. The dependent variable is the tire's tread depth.
Independent Value | The unit of the measuring quantity that is defined for the independent variable of the measurement.
Follow-up Order | The code of the follow-up service order that the inspection was part of.
Follow-up Activity | The code of the follow-up activity.
Commands | Description
Inspections | Starts the Inspections (tssoc2550m000) session.
Apply | Click this button to search for the list of inspections that has been conducted on a serialized item based on the search criteria. Enter the relevant details in the following To and From fields: Measurement Independent Value Dependent Value Follow-Up Activity Registration Time
Delete Serialized Item Inspections History | Starts the Delete Serialized Item Inspections History (tssoc2250m000) session.