| EBOM Copy Data (tiedm1120m000) |  |
| Use this session to generate and maintain the copy data for a single-level engineering BOM. You can alter the details of the data of a particular line in the EBOM Copy Data (tiedm1120m000) details session. You can also use this session to change data generated by the Generate EBOM Copy Data (Multilevel) (tiedm1230m000) session and the Generate EBOM Copy Data by MBC (tiedm3235m000) session. Data selection To create the copy data for a single-level of a BOM, select a parent E-item of a particular revision from which the data originates, and a parent item to which the data is to be copied. The parent item is the item at the next higher level in the BOM structure compared to the component(s) for which you record the copy data. If a relationship does not already exist between the E-items and items, ERP LN generates the link when you save the data. To copy the data You can copy the data you generate in this session with the Finalize Engineering Data (tiedm3240m000) session. If you want to copy only the data that you see in the current view, you can select the Copy engineering data option on the Specific menu (CTRL+SHIFT+X). Specific menu options In the Specific menu, you can start the following sessions: Generate EBOM Copy data If you find that the copy data is different from the EBOM, you must use this option to update the copy data for the single-level BOM. If you want to copy a multilevel EBOM, use the Generate EBOM Copy Data (Multilevel) (tiedm1230m000) session. Note that the lines are not actually copied. Only the copy data is updated. Check Consistency If the copy data of the EBOM and the production BOM differs, ERP LN displays a message stating in which BOM position (line) the discrepancy occurs. to display or print the inconsistency, use one of the following sessions: The EBOM and PBOM Consistency (tiedm1520m000) session. The Print EBOM and PBOM Consistency (tiedm1470m000) session. Finalize Use this option to copy data from a single-level EBOM to a production BOM. ERP LN copies data in the current view. You must do one of the following: Select Automatic in the Update Method E-Item Relation field in the Item - General (tcibd0101s000) session. You can alter that field for a range of items in the Update Engineering Relationship (tiedm3220m000) session. First create a relationship in the Engineering Item - Item Relationship (tiedm1101m000) session. If you want to copy a multilevel EBOM, use the Generate EBOM Copy Data (Multilevel) (tiedm1230m000) session followed by the Finalize Engineering Data (tiedm3240m000) session. Copy Engineering Item to Item ERP LN starts the Copy Engineering Item to Item (tiedm1201m000) session. Use Up and Alternative Materials in EBOM Copy Data ERP LN starts the Use Up and Alternative Materials in EBOM Copy Data (tiedm2125m000) session. Related topics Engineering data management summary Engineering BOMs Copying E-items to items Overview of reference designators Procedure for linking reference designators in the EBOM Reference designators and MBCs To define alternative materials
Fields | Description
Engineering Item | Enter the single-level EBOM's parent E-item that you want to copy.
E-Item Revision | Enter the parent E-item revision of the single-level EBOM that you want to copy.
E-Item Revision | The description or name of the code.
Main Item | Enter the parent item of the target production BOM (that is, the BOM to which you want to copy the single-level EBOM).
Position Number | The target position number of the PBOM line.
Component Type | Defines whether the component is an E-Item or Item.
Component | The source component in the EBOM line.
EBOM Copy Method | The copy method used by ERP LN for copying the EBOM to the production BOM. Allowed values No Copy Action Copy E-Item to Item NonProj Item to Proj Item EBOM to PBOM Only Possible Values Related topics Engineering BOMs
Finalized to Position | The line number of the target production BOM, that is, the BOM to which you want to copy the data.
Sequence Number | The sequence number of the target BOM.
Item Category | The item category of the target item.
To Item | The target component item in the PBOM, which is the BOM line to which you want to copy the EBOM line. Related topics Engineering BOMs Copying E-items to items
E-BOM Text | If this check box is selected, a text is present.
Length | The length of the component in the EBOM line. Note Length can also be used to calculate Net Quantity: Net Quantity = Length x Width x Number of Units.
Width | The width of the component in the EBOM line. Note Width can also be used to calculate Net Quantity: Net Quantity = Length x Width x Number of Units.
Number of Units | The number of times the component occurs in the length (or area). For a physical item, this is equal to the number of units in the length or area defined. It can also be used to calculate Net Quantity: Net Quantity = Length x Width x Number of Units.
Net Quantity | The net quantity of the component in the EBOM line. This is the amount of the component item used in the E-item. This can be calculated by multiplying the Number of Units, Length, and Width. Example: If ten units of a component 2 cm long and 3 cm wide are specified, the net quantity is calculated as 60. If the width is not specified, the net quantity is 20. Note You cannot define negative net quantities in the Engineering Data Management module. Related topics Scrap and yield
Extra Information | From the Extra Information field in the Engineering BOM (tiedm1110m000) session. You can use this field to enter a short note about the item or the BOM line.
Description | The description or name of the code.
E-Item Copied | If this check box is selected, then the E-item has already been copied to an item.
E-Item Copied | The date on which the E-item was copied to an item.
EBOM Copied | If this check box is selected, the single-level EBOM has already been copied to a production BOM.
EBOM Copied | The date on which the EBOM was copied to a PBOM.
Description | The name of the parent E-item revision of the single-level EBOM that you want to copy.
Quantity Independent | If this check box is selected, the E-item's net quantity is copied to update the scrap quantity in the BOM. If this check box is cleared, the E-item's net quantity is copied to update the net quantity of the BOM.
Commands | Description
Generate EBOM Copy data | Click to generate EBOM copy data for the selection you have made in this session. If you want to generate copy data for the entire BOM, use the Generate EBOM Copy Data (Multilevel) (tiedm1230m000) session.
Finalize | Click to copy the data you have defined in this session.
Use Up and Alternative Materials in EBOM Copy Data | Click to start the Use Up and Alternative Materials in EBOM Copy Data (tiedm2125m000) session.