| Cluster - Lines (List) (tsbsc1110m100) |  |
| Use this session to list and maintain all cluster configurations. Example A machine consists of two engines (configurations), each of which has the code CF6, and the machine belongs to your business partner MACH Industries (MACHI). The name of this cluster is CF6 machine MACHI. The code of the first engine (configuration) can be CF6/101, and the code of the second engine (configuration) CF6/102. Note You can use the Sort by command on the View menu to choose the way you want to display the cluster data. On the Specific menu, you can choose: Create Physical Breakdown- Enables you to generate a physical breakdown structure from one of the following: Item breakdown As-built structure ASCII file Project-breakdown structures Physical Breakdown- Enables you to view or maintain the multilevel or single-level parent-child relations between serialized items that form a physical breakdown. A physical breakdown is defined for a configuration, which enables you to view the configuration's built-up structure and as-maintained structure. Item Breakdown- Enables you to view or maintain the parent-child relations between items that form an item breakdown. Item Details- Starts the Serialized Items (tscfg2100m000) session. Activate Cluster Configurations- Starts the Activate Cluster Configurations (tscfg2210m500) session, which enables you to switch the status of multiple configurations to Active in one run.
Fields | Description
Cluster | The cluster to which the configuration is linked.
Cluster | The description or name of the cluster.
Line | The number identifying the configuration.
Item | The item(s) you select to make up the configuration. Two possibilities: One serialized item. The configuration then consists of the serialized item, and the items in its physical breakdown. In this case, the value of the Number of Items field will be one and unchangeable. Any quantity of an anonymous item. In this case, you can specify the quantity in the Number of Items field. The configuration consists of the anonymous item(s), and the items in its item breakdown.
Serial Number | If you link a serialized item to this cluster, enter the item's serial number in this field. Note This field is not available if you have entered a quantity greater than the value in the Number of Items field.
Description | The description or name of the item(s) belonging to the cluster.
Number of Items | The number of items in this cluster's configuration line. Note This field is not available if you select a serialized item for the configuration (in this case the default value will be one).
Status | The status of the (serialized) item in the cluster.
Status Start Time | The time when the Status field is set or changed.
Planned Until Time | The time until which maintenance activities are actually planned for the cluster configuration. Note The planned until time date must fall within the effective period of this cluster configuration. If the cluster is linked to an active contract, you cannot modify this time manually before or during the effective period of the contract. However, you can modify the time to a date after the expiry date of the contract.