| Defining blocking reasons for QM |  |
| Quality Management uses blocking reasons to communicate with the Shop Floor Control module in Manufacturing. By means of these blocking reasons Quality Management can block certain actions that you can carry out on operations. For this purpose you must define 5 blocking reasons. The following procedure ensures that each blocking reason has the correct type. Step 1. Define blocking reasons Define 5 blocking reasons in the Blocking Reasons (tisfc2100m000) session with the following characteristics:
Blocking reason | (1) | (2) | (3) | (4) | (5)
Use in OM | Y | Y | Y | Y | Y
Block Quantity Completed | Y | Y | N | N | N
Block Quantity Rejected | Y | Y | N | N | N
Block Quantity to be Inspected | N | N | Y | Y | Y
Blocked for Completion | Y | N | N | Y | N
Y (Yes) indicates that you must select the check box. Step 1. Define blocks on operations Use these blocking reasons to define the blocks on operations in the Quality Management Parameters (qmptc0100m000) session. Enter the first three blocking reasons in the Block on Operation group box: Active Inspections: blocking reason (1) Inactive Inspections: blocking reason (2) Processed Inspections: blocking reason (3) Enter the last two blocking reasons in the Block on Completion of Operation group box: Active Inspections: blocking reason (4) Inactive Inspections: blocking reason (5) Related topics Blocking operations Using QM for manufacturing operations |