| Inspection Order Header History (qmptc3505m000) |  |
| Use this session to display the inspection orders for a specific origin order. In the Inspection Order Header History (qmptc3505m000) details session you can view the inspection orders' details like test type, sample size, and acceptable quality level. Related topics Standard inspections
Fields | Description
Origin | An integrated module or package to which an (inspection) order is related.
Origin Order | The order number of the inspection's origin.
Item | In ERP LN, the raw materials, subassemblies, finished products, and tools that can be purchased, stored, manufactured, sold, and so on. An item can also represent a set of items handled as one (kit), or exist in multiple product variants (generic item). You can also define nonphysical items, which are not held in inventory but can be used to post costs or to invoice services to customers. Examples of nonphysical items: Cost items (for example, electricity) Service items Subcontracting services List items (menus/options)
Item Description | Displays the description of the item.
Order Quantity | The physical quantity in which an item or good is managed. For example, a quantity of wood can be expressed as a length by using the unit of one meter, or as a volume by using the unit of one cubic meter.
Order Quantity | Displays the order quantity.
Order | An order used to structure the inspection of products that are purchased, produced, or sold.
Test Type | Specification of the way in which the samples are taken from the order quantity.
Sample Size | The total quantity of samples from the order quantity to be tested, expressed in the unit of the sample size. The sample size can be entered as a fixed quantity or as a percentage of either the order quantity or the frequency (if you selected Continuous Sampling as test type).
Sample Unit | The unit of the sample size.
Frequency | The interval between two samples, expressed in the frequency unit. Explanation: A new sample of 10 pieces is drawn for every 100 pieces. In this case there will be 11 samples of 10 pieces. Example
Sample | 10 pieces
Frequency | 100 pieces
Order quantity | 1150 pieces
Percentage | Displays the percentage of the sample as part of Methodology.
Sample Unit | Displays the Sample Unit as part of the Methodology.
Acceptable Quality Level | The minimum percentage of a test sample that must be approved to have the entire item quantity approved. For instance, if the AQL is set to 90 and the percentage approved lies below that figure, the entire quantity is rejected.
Inspection Order Text | Displays text related to Inspection Order Header History.
Line | The position number on the order to which the inspection order is linked. This can be the position number of the sales order line, the position number of the purchase order line, the position number in the BOM.
Operation | One of a series of steps in a routing that are carried out successively to produce an item. The following data is collected during a routing operation: The task. For example, sawing. The machine used to carry out the task (optional). For example, sawing machine. The place where the task is carried out (work center). For example, woodwork. The number of employees required to carry out the task. This data is used to compute order lead times, to plan production orders and to calculate cost prices. A quality inspection took place during or after this operation.
Sequence | The sequence number of the inspection order on the basis of which characteristics are tested on different samples.
Inspection | Displays a list of the inspection order lines generated for a particular inspection order. These lines will correspond to characteristics maintained for each of the test groups that are linked to the Quality ID.
Inspection | Displays the sequence of the inspection that is carried out.
Handling Unit | It is a structure of packaging materials, or a part of such structure, used to pack items. Note A handling unit includes the following attributes: 1)Identification Code. 2)Packaging item(optional). 3)Quantity of packaging items (optional). Important! If you link an item to a handling unit, the item is packed by means of the handling unit. The packaging item refers to the type of container or other packing material of which the handling unit consists. For Example: By defining a packaging item such as wooden crate for a handling unit, you specify that the handling unit is a wooden crate.
Quality ID | The conditions that determine the generation of inspection orders, and how the inspections are carried out. A quality combination links the following information: The module or package that is the origin of the quality inspections. The item or quality group to which the quality inspections apply. The quality requirements that must be met (defined in the quality ID).
Quality ID | Displays the Quality ID and description.
Test Group | The definition of how often you take samples to test an order quantity, and what the sample size is.
Order Date | The date on which the inspection order is created.
Completion Date | The date on which all inspection order lines are completed. This date is updated automatically in the Complete and Process Inspection Orders (qmptc1202m000) session, and cannot be entered manually.
Commands | Description
Samples History | Displays Samples History option under Specific in File Menu. Click Samples History to display Samples History (qmptc3510m000)session.
Inspection Order Lines History | Displays Inspection Order Lines History under Specific in File Menu. Click Inspection Order Lines History to display Inspection Order-Lines History(qmptc3506m000)session.