| Storage Inspection - Inspection Orders History (qmptc2505m000) |  |
| Use this session to display the inspection orders for storage inspections that are carried out in the past. The inspection orders are listed by item. Related topics Storage inspections
Fields | Description
Completion Date | The date on which all inspection order lines are completed. This date is updated automatically in the Complete and Process Inspection Orders (qmptc1202m000) session and cannot be entered manually.
Order | An order used to structure the inspection of products that are purchased, produced, or sold.
Sample Unit | The unit of the sample size.
Frequency | The interval between two samples, expressed in the frequency unit. Explanation: A new sample of 10 pieces is drawn for every 100 pieces. In this case there will be 11 samples of 10 pieces. Example
Sample | 10 pieces
Frequency | 100 pieces
Order quantity | 1150 pieces
Item | In ERP LN, the raw materials, subassemblies, finished products, and tools that can be purchased, stored, manufactured, sold, and so on. An item can also represent a set of items handled as one (kit), or exist in multiple product variants (generic item). You can also define nonphysical items, which are not held in inventory but can be used to post costs or to invoice services to customers. Examples of nonphysical items: Cost items (for example, electricity) Service items Subcontracting services List items (menus/options)
Order Date | The date on which the inspection order is created.
Acceptable Quality Level | The minimum percentage of a test sample that must be approved to have the entire item quantity approved. For instance, if the AQL is set to 90 and the percentage approved lies below that figure, the entire quantity is rejected. Related topics Examples of the Acceptable Quality Level (AQL)
Percentage | The sample size is the total quantity that is to be tested. In this field, the sample size is expressed as a percentage of either the order quantity or the frequency (in case you selected Continuous Sampling as the test type).
Quality ID | The conditions that determine the generation of inspection orders, and how the inspections are carried out. A quality combination links the following information: The module or package that is the origin of the quality inspections. The item or quality group to which the quality inspections apply. The quality requirements that must be met (defined in the quality ID).
Sample Size | The total quantity of samples from the order quantity to be tested, expressed in the unit of the sample size. The sample size can be entered as a fixed quantity or as a percentage of either the order quantity or the frequency (if you selected Continuous Sampling as test type).
Sequence | The sequence number identifies the storage inspections for a particular item.
Test Group | The definition of how often you take samples to test an order quantity, and what the sample size is.
Test Type | Specification of the way in which the samples are taken from the order quantity.
Order Quantity | The quantity for which the inspection is required. Consequently, the result of the inspection order concerns the quality of this quantity.