| Characteristics -Tests (qmptc0105m000) |  |
| Use this session to display the tests that are used to inspect characteristics. Multiple tests can be used to test a single combination of aspect and characteristic. Related topics You can create and/or maintain tests in the details session. Master data, quality management
Fields | Description
Aspect | A part of an item. For example, a bolt can have the aspects head and tail. An aspect can have one or more characteristics. For example, a head can have a diameter and a length, and a tail can have a diameter and a color.
Characteristic | A reference to a particular quality or distinctive mark of an item or an item part/component. For example, diameter, length, weight.
Test | An examination or check done on a characteristic. You can link one or more tests to a characteristic.
Test Unit | The unit that applies to the test. For example, meter, liter, or kilogram..
Result Type | The following result types are available:
Test Standard | The standard normally used for the test. For example, a DIN standard.
Destructive Test | If this check box is selected, the test is destructive and the item cannot be used after testing. If this check box is cleared, the test is not destructive and the item can be used after testing.
Skill | The specific know-how or technical expertise that an engineer must have to carry out activities. For example, knowledge of electricity, specific equipment, and so on.
Test Area | The physical location where tests take place.
Employee | The employee who performs the test for this characteristic.
Instrument | A tool that is used during quality tests to measure particular characteristics of an item. Example
Instrument | acidimeter
Characteristic | pH value