| Storage Inspection Orders (qmptc2100m000) |  |
| Use this session to define and modify storage inspection orders for an item. If you double-click an inspection order, you can view the details in the Inspection Orders (qmptc1100m000) session. Note You can only create or modify inspection orders if the Status field is Free or Active (see the Item - Storage Inspections (qmptc2120m000) session), and if no order lines have an Order Line Status greater than Active (see the details session of the Inspection Order - Lines (qmptc1101m000) session). Related topics Storage inspections
Fields | Description
Item | In ERP LN, the raw materials, subassemblies, finished products, and tools that can be purchased, stored, manufactured, sold, and so on. An item can also represent a set of items handled as one (kit), or exist in multiple product variants (generic item). You can also define nonphysical items, which are not held in inventory but can be used to post costs or to invoice services to customers. Examples of nonphysical items: Cost items (for example, electricity) Service items Subcontracting services List items (menus/options) Note Standard items are expressed in an item code. Segmented items consist of a project code segment and an item base segment (the item code of the customized item). The segments an item can consist of are defined in the Item Code Segmentation (tcibd0500m000) session.
Sequence | The sequence number of the inspection order on the basis of which characteristics are tested on different samples.
Order | An order used to structure the inspection of products that are purchased, produced, or sold.
Test Type | Specification of the way in which the samples are taken from the order quantity. Allowed values Possible Values
Frequency | The interval between two samples, expressed in the frequency unit. Explanation: A new sample of 10 pieces is drawn for every 100 pieces. In this case there will be 11 samples of 10 pieces. Example
Sample | 10 pieces
Frequency | 100 pieces
Order quantity | 1150 pieces
Note You cannot continue the inspection procedure when your order quantity is less than the frequency quantity(for example, when your order quantity is 40, and your frequency quantity is 50). In such a case, no samples can be generated, and you must decrease the frequency quantity.
Sample Size | The sample size is the total quantity of all samples which are to be tested out of the order quantity, expressed in the unit of the sample size. In this field, it is expressed as a fixed quantity.
Unit | The unit of the sample size.
Acceptable Quality Level | The minimum percentage of a test sample that must be approved to have the entire item quantity approved. For instance, if the AQL is set to 90 and the percentage approved lies below that figure, the entire quantity is rejected.