| Shared Work Center Utilization by Day Overview (tisfc1509m000) |  |
| Use this session to display an overview of capacity utilization for a shared work center for one day. You can see, for each order, the time and quantity that it is planned to occupy the work center. You can only use this session if you have selected Automatic or Manual in the Update Method Day Utilization field of the Shop Floor Control Parameters (tisfc0100s000). Before you can use this session you must run the Build Utilization (tisfc0201m000) session (in the work center's company). You must select Automatic or Manual in the Update Method Day Utilization field and Automatic or Manual in the Update Method Week Utilization field in the Shop Floor Control Parameters (tisfc0100s000) session to update the plans on a daily basis. In the Shared Work Center Relationships (tirou3100m000) session, you defined the Percentage Capacity of the primary work center allocated to the current secondary work center. That determines the capacity of the secondary work center. If the primary work center has a capacity of 80 hours per week and the current secondary work center has a Percentage Capacity of 50%, its capacity will be 40 hours. Related topics Shared work centers Production orders - functional overview
Fields | Description
Work Center | The shared work center whose planned capacity utilization you want to see.
Company | The company of the shared work center.
Date | The day for which the planned capacity utilization for the work center is displayed.
Work Center | The secondary work center whose planned capacity utilization you want to see.
Normal Man Capacity | The secondary work center's normal capacity expressed in man hours. The normal capacity is calculated from the following fields in the Work Centers (tirou0101m000) session:
    Number of Operators	* Basic Day Capacity by Resource Unit.
Available Man Capacity | The secondary work center's available capacity expressed in man hours. The available capacity is calculated as follows:
    Capacity in	calendar * Number of Operators * Percentage Shared Capacity.
Where:
    Capacity in	calendar = Calendar Time * Efficiency Factor * Percentage Capacity.
Calendar time = end date - start date (for one record in the actual calendar). Efficiency Factor = working time / clock time. Percentage Shared Capacity = the percentage allocated to the shared secondary work center. In case of a primary shared work center or no shared work center, the percentage is 100%. Related topics How to calculate available capacity
Total Man Hours | An aggregation of the secondary work center's remaining/outstanding operation hours for the specified period expressed in man hours. Because these are remaining hours, the spent hours booked in People, are not counted.
Normal Machine Capacity | The secondary work center's normal capacity expressed in machine hours. The normal capacity is calculated from the following fields in the Work Centers (tirou0101m000) session:
    Number of Machines	* Basic Day Capacity by Resource Unit.
Available Machine Capacity | The secondary work center's available capacity expressed in machine hours. The available capacity is calculated as follows:
    Capacity in	calendar * Number of Machines * Percentage Shared Capacity.
Where:
    Capacity in	calendar = Calendar Time * Efficiency Factor * Percentage Capacity.
Calendar time = end date - start date (for one record in the actual calendar). Efficiency Factor = working time / clock time. Percentage Shared Capacity = the percentage allocated to the shared secondary work center. In case of a primary shared work center or no shared work center, the percentage is 100%. Related topics How to calculate available capacity
Total Mach. Hours | An aggregation of the secondary work center's remaining/outstanding operation hours for the specified period expressed in machine hours. Because these are remaining hours, the spent hours booked in People, are not counted.
Work Center | A work center that does not have any physical resources and cannot be modeled in a routing. It is used for capacity planning and displays the total capacity requirements of the shared work centers. The work is actually carried out in shared secondary work centers, which can be in the same or a different logistical company than the primary work center. This enables you to plan and carry out work in several different logistical companies (if you define several secondary work centers) without having to use sales orders and purchase order.
Company | The company of the primary work center.
Normal Man Capacity | The primary work center's normal capacity expressed in man hours. The normal capacity is calculated from the following fields in the Work Centers (tirou0101m000) session:
    Number of Operators	* Basic Day Capacity by Resource Unit.
Available Man Capacity | The primary work center's available capacity expressed in man hours. The available capacity is calculated as follows:
    Capacity in	calendar * Number of Operators * Percentage Shared Capacity.
Where:
    Capacity in	calendar = Calendar Time * Efficiency Factor * Percentage Capacity.
Calendar time = end date - start date (for one record in the actual calendar). Efficiency Factor = working time / clock time. Percentage Shared Capacity = the percentage allocated to the shared secondary work center (in case of a primary shared work center or a no shared work center, the percentage is 100%. Related topics How to calculate available capacity
Total Man Hours | An aggregation of the primary work center's remaining/outstanding operation hours for the specified period expressed in man hours. Because these are remaining hours, the spent hours booked in People, are not counted.
Normal Machine Capacity | The primary work center's normal capacity expressed in machine hours. The normal capacity is calculated from the following fields in the Work Centers (tirou0101m000) session:
    Number of Machines	* Basic Day Capacity by Resource Unit.
Available Machine Capacity | The primary work center's available capacity expressed in machine hours. The available capacity is calculated as follows:
    Capacity in	calendar * Number of Machines * Percentage Shared Capacity.
Where:
    Capacity in	calendar = Calendar Time * Efficiency Factor * Percentage Capacity.
Calendar time = end date - start date (for one record in the actual calendar). Efficiency Factor = working time / clock time. Percentage Shared Capacity = the percentage allocated to the shared secondary work center. In case of a primary shared work center or a no shared work center, the percentage is 100%. Related topics How to calculate available capacity
Total Mach. Hours | An aggregation of the primary work center's remaining/outstanding operation hours for the specified period expressed in machine hours. Because these are remaining hours, the spent hours booked in People, are not counted.
Start Time | The production date to which the utilization applies.
Machine | The machine on which the operation is carried out.
Production Order | The planned production order.
Routing | The routing of the planned production order at the shared work center.
Operation | The operation carried out at the shared work center.
Task | The task carried out at the shared work center.
Quantity Planned | The quantity you plan to produce in the current operation at the shared work center.
Man Hours | The man hours needed to carry out the operation.
Machine Hours | The machine hours needed to carry out the operation.
Physical Location | The location where the operation is carried out on the shop floor. You can also use this field to enter other information about the production order.
SFC Order Group | The SFC order group to which the production order belongs. Related topics Order grouping
Item | The end-item produced by the production order.