| Order-specific inspections |  |
| Inspection orders are used to structure the inspection of products. They are generated based on quality combinations. This means that each item to which a certain quality combination applies is inspected in the same way. You can deviate from this by means of order-specific inspections. Order-specific inspection data is the copied quality combination (that is, standard inspection data) that you can modify and change for a specific order in a specific situation. Order-specific inspection data is generated when you select the Order-Specific Inspection Data parameters in the Quality Management Parameters (qmptc0100m000) session. Procedure to generate order-specific inspections Step 1. Use the Specific Orders - By Origin (qmptc0149m000) session to provide an overview of the origins and the related orders. Note: If the QM Implemented parameter in the Quality Management Parameters (qmptc0100m000) session is selected, the Specific Orders - By Origin (qmptc0149m000) session can also be started from other modules. Step 2. Start the Specific Order - Inspection Orders (qmptc0550m000) session from the Specific menu in the Specific Orders - By Origin (qmptc0149m000) session. You can change, add, or delete order-specific inspection orders in the Specific Order - Inspection Orders (qmptc0150m000) details session. Step 3. Start the Inspection Order - Lines (qmptc0151m000) session from the Specific menu in the Specific Order - Inspection Orders (qmptc0550m000) session. You can now define the order-specific inspections lines. Each line represents a characteristic that was defined in the Test Group - Characteristics (qmptc0137m000) session. The order-specific inspection order is now generated. The rest of the inspection procedure is the same as that described from step 2 (drawing samples) in the Standard inspections online manual topic. Related topics Standard inspections |