| Device Data (ttaad3100s000) |  |
| Use this session to define the various output devices that are used in an ERP LN environment. The device types to which a print request can be sent in ERP LN are: Printer Logical printer Append to file Rewrite file Direct Screen Windows Printer Windows Server Printer Infor Enterprise Report Printer Microsoft Reporting Services For every print request to a ERP LN Printer device an intermediate print file "tmpxxxxx" is stored in directory $BSE/tmp. Note For a Windows printer the intermediate print file "tmpxxxx.bpf" is not stored in directory $BSE/tmp, but the file will be transferred to the users PC and printed by the ERP LN Windows print program BWPrint. The session is divided into three parts. You can specify: General device data: for each device you must enter basic properties such as the name, description, type, and character set. Data related to (physical) printers Data related to append and rewrite files Depending on the device type, you must skip or fill certain fields. For example, if you define a physical printer, you can skip the file-related fields. Related topics Device Management Procedure Device Management
Fields | Description
Device | The output device code. This device code is a unique code that identifies a printer. You can choose a unique name for a device, however the name SMTP is reserved for Microsoft Outlook to send the print file directly to e-mail and the name FAX is reserved to print directly to a FAX device. This code is used by a user to send a report to an output device. Examples: ASCII (ASCII file) NOTEPAD (NOTEPAD file) D (Display Device) D66 (Display Device 66 lines per page) WINDOWS (Default Windows printer) pnl0133L (Unix printer pnl0133 Landscape) pnl0133P (Unix printer pnl0133 Portrait) pnl0133D (Unix printer pnl0133 Direct) pnl0133W (Windows printer pnl0133)
Description | The description of the output device. It is a good manner to specify the location of the printer if possible. Examples: IBM Printer in building X HP Laserjet in room Y Default Windows printer Rewrite to file ASCII format Print to Excel sheet Print to file HTML format Print to Business Objects Enterprise
Device Type | The type of output device. Possible values
Locale | Specifies the name of the Tools Super Set locale. A locale is a collection of the TSS character set definition, the NLS locale for the system and minimum and maximum values for form and database fields. Each locale uses a specific range of (multi-byte) characters of the Tools Super Set (TSS). The user locale belonging to the user who makes a print request, must be equal to the print locale. If a user tries to select a print device with a locale different from the user locale, the ERP LN system sends an error message and the report will not be printed. Examples: ISO-8859-1 (Western Europe - 8 bit) GB-SUN (Simplified Chinese Sun) HEBREW-AIX (Hebrew IBM AIX) Note If you have a Unicode installation, Infor advises you to leave the Locale field empty if you have chosen Windows Printer as the device type. In that case BWPrint automatically uses the locale of the Windows system.
Intermediate File in XML Format | If this check box is selected, the intermediate print file in $BSE/tmp is stored in XML format. XML files can be reused by other applications, for example Business Objects Enterprise. See the Argument field for details about printing a ERP LN Report via Business Objects Enterprise.
Driver | The printer driver's code. A printer driver is a file that contains settings, such as control characters, escape sequences, and so on, for a specific printer. The driver specification is only applicable for Unix printers, printer type "Printer" or "Direct". For a Windows printer, the printer driver is stored on a local PC or on a Windows Printer Server. The Unix printer drivers can be found on the Unix file system in directory $BSE/lib/printinf. This directory contains several one-character sub-directories for each Printer Supplier, see example list below: Directory c - Canon Directory e - Epson Directory h - HP (Hewlett Packard) Directory i - IBM Directory m - Mannesmann Directory s - Siemens Example printer drivers: hp_lj4 ( HP Laserjet 4 Portrait printer) hp_lj4_lndsc (HP Laserjet 4 Landscape printer)
Device Queue | The name of the printer as used by the Unix printer spooler. The value in the Device Queue field depends on the value in the Device Type field: If Device Type is Printer then the Device Queue is the name of the printer as used by the Unix printer spooler (for example, pnl0133) If Device Type is Direct the print request is not handled by the printer daemon. Therefore the Device Queue is a UNIX print command with parameters to carry out the print directly (for example, lp -dpnl0133 -n%d -s %s). If Device Type is Windows Printer then the Device Queue is the name of the Windows printer (for example: \\SRV_NLD_DEV2\PNL0133) . If this field is <empty> the default Windows printer of the user is used. For all other Device Types the Device Type field is disabled
Paper Type | The paper type loaded in the printer's paper tray. The Paper Type specification is only applicable for the following Device Type: Printer Logical printer Windows printer
Left Margin | The left margin for reports sent to a printer. The Left Margin specification is only applicable for the following Device Types: Printer Windows printer Note When you print a report, the Select Device (ttstpsplopen ) session suggests a left margin. This suggested margin is calculated as follows: `suggested margin = the device margin specified in this field + the report's left margin specified in the Reports (ttadv3130s000) session`
Form Feed Every Page | Specify whether a form feed is sent after each report page. The Form Feed Every Page check box is only applicable for Device Type: Printer. If this check box is selected, a form feed is sent to the printer at the end of each report page. If this check box is cleared, no form feed is sent at the end of the report page. If the page length of the report does not correspond with the page length of the paper type, the report page will be printed over several printer pages.
Driver | The Unix printer driver that must be used for device types Rewrite file and File append. See for details: Driver.
Shell Command | The program, at operating system level, which is executed before the output is (re) written to a file. For example, this program can be a conversion program to filter the input data.
4GL Program | The 4GL Program field is used to define the name of a ERP LN 4GL program, that is used to convert the output of an ERP LN Report to another format. For example to HTML format. This 4GL Program field is only applicable for the Device Types: Rewrite file and Append to file. The most important available ERP LN 4GL program to mention here is the conversion program: ttstpconv. This program is able to convert a ERP LN Report to several formats, for example HTML, RTF, Postscript, etc. To specify the type of conversion to be done, the program uses Program Arguments, that can be specified in the Argument field. Another available ERP LN 4GL Program is the CMF (Common Messaging Facility) Print Utility: ttcmfprint. The ttcmfprint utility is able to send a ERP LN Report to an E-mail address, Fax etc. The ttcmfprint utility always converts the report to RTF format. See the Argument field for details about the Conversion Programs.
Argument | The arguments you can specify here are dependent on the ERP LN 4GL Program, that is specified in the 4GL Program field. See table below for the possible arguments:
4GL program | Argument | Description
ttstpconv | ascii | ASCII (American Standard Code for Information Interchange) format
ttstpconv | html | HTML (HyperText Markup Language) format
ttstpconv | rtf | RTF (Rich Text Format) format (Portrait)
ttstpconv | rtf_landscape | RTF (Rich Text Format) format (Landscape)
ttcmfprint | outlook | The report is sent to E-mail recipients using MS Outlook If using argument outlook then it is mandatory to specify the Device code as SMTP (Simple Mail Transfer Protocol) The E-mail addresses must be specified in the Path field
ttcmfprint | fax | The report is sent to FAX numbers If using argument fax then it is mandatory to specify the Device code as FAX Fax numbers must be specified in the Path field
<empty> | XML | XML (Extensible Markup Language) used for Business Objects Enterprise If using argument XML then it is mandatory to select the check box Intermediate File in XML Format
<empty> | XML -PRS | The report is sent to Production Reporting Services (PRS). If using argument XML then it is mandatory to select the check box Intermediate File in XML Format On a PRS device, you can only print reports that are enabled for Production Reporting, and that are ready for data processing. For details on PRS, and on the setup of a PRS device, refer to the Business Intelligence 1.3 for ERP LN Production Reporting Services User’s Guide.
<empty> | XML -PDF | The report will be converted to PDF format. If using argument XML then it is mandatory to select the check box Intermediate File in XML Format
<empty> | server=<printer server name> port=<port number for ES Reporting Service > | The report is sent to a Windows Server Printer. For details, refer to Windows printer devices. Note: You can leave the Argument field blank for a Windows Server Printer, if ERP LN runs on a Windows server. When you send a report, BWPrint is started on the ERP LN server.
<empty> | XML -RPT | The report is sent to the ERP LN Report Viewer. For more information, refer to To create a Report Viewer device for session-based reports. Note: You can only use the Report Viewer device to print reports with an XML report design.
| -printer | When using direct print the report is not shown in the report viewer but directly sent to the printer. Prints the report to the default printer of the user. Only possible when there is a UI, so not possible when in job mode.
| -printer <printer> | Prints the report to the specified printer. Not possible on UNIX in job mode.
| -device <windows printer device> | Prints the report to the specified Windows Printer device. It uses the Device Queue of the Windows Printer device. Not possible on UNIX in job mode.
| -device <windows server printer device> | Prints the report to the specified Windows Server Printer Device. It uses the Device Queue of the Windows Server Printer device. In the argument of the Windows Server Printer device the server and port number to connect to the Infor ES Reporting Service have to be specified.
The arguments ascii, html and rtf can be appended with :<Client program> to start a program on the client PC for editing the ERP LN Report and can be appended with \<Unix shell script> to filter or modify the Report output file, see the examples in the table below:
Example | Explanation
ascii | Create ASCII file
ascii: | Create ASCII file and start notepad (default)
ascii:notepad | Create ASCII file and activate notepad
ascii\mfax %s | Create ASCII file and send file to mfax
ascii\mfax %s:notepad | Create ASCII file, send file to mfax and activate notepad
ascii:excel | Create ASCII file and activate MS excel
ascii:winword | Create ASCII file and activate MS Word
rtf:winword | Create RTF file and activate MS Word
html:winword | Create HTML file and activate MS Word
html:iexplore | Create HTML file and activate Internet Explorer
postscript | Create PostScript file. Use a PostScript printer to print the file
wp50 | Create WordPerfect 5.0 file
uni | Create Uniplex file
For some arguments you can specify Parameters behind the argument, see table below:
Argument | Parameter | Mandatory | Explanation
ascii | -u | No | LSB UNICODE (16 bit) format
ascii | -umsb | No | MSB UNICODE (16 bit) format
ascii | -win32 | No | Windows 3.2 format
html | -c <company> | No | Display company name on each HTML page
html | -g <logo.gif> | No | Display company logo on each HTML page. The company logo must be in the same directory as the HTML report produced in order for the logo to be displayed with the report.
html | -f <fontsize> | No | Fontsize
XML | server <server name> | Yes | The name of the Business Objects Enterprise server
XML | port <port number> | Yes | The port number on the Business Objects Enterprise server
In the table below some examples of the arguments and their parameters are shown:
Example | Explanation
ascii -u | Create ASCII file in LSB UNICODE (16 bit) format
ascii -umsb | Create ASCII file in MSB UNICODE (16 bit) format
ascii -win32:notepad | Create ASCII file in Windows 3.2 format and activate notepad
html -c "MPC Global" -g "CMP.gif" -f 12 | Create HTML file with company name and logo, fontsize 12
html -c "MPC Global" -g "CMP.gif" -f 12:iexplore | Create HTML file with company name and logo, fontsize 12 and activate Internet Explorer
XML server=cnl01234 port=8999 | Create XML file and send the file to Business Objects Enterprise server cnl01234 on port number 8999
Path | The content of this field depends on the Device Type. See the table below.
Device Type | Content of Path field
Rewrite file Append to file | The (default) path of the file you want to create. If the Conversion Program field contains ttcmfprint then the Path field contains the address where the file should be sent. For example, an email address or a fax number. In case of multiple recipients, the field contains multiple addresses separated by semicolons ";". For example:
Device | Conversion Program | Argument for Conversion Program | Path
SMTP | ttcmfprint | outlook | jsmith@company-x.com; gbush@president.gov
FAX | ttcmfprint | fax | +31 342123456; +40 98765432
Printing redesign based on RTF specification 1.9.1 (Used by Microsoft Word 2007/Word 12)
Device | Conversion Program | Argument for Conversion Program | Path
RTF | ttstpconv | RTF:Winword.exe %s | ${HOME}/rtf
RTFA4 | ttstpconv | RTFL:Winword.exe %s A4 L9 R3 | ${HOME}/rtf
RTFLTC | ttstpconv | RTF:Winword.exe %s LTC L3 R3 | ${HOME}/rtf
RTFLT | ttstpconv | RTF:Winword.exe %s LT L3 R3 | ${HOME}/rtf
Infor Enterprise Report Printer | The URL to connect to the report renderer on the Infor Reporting Services server. The URL has this format: http://< Infor Reporting Services server>:<port>/IRServices/reportRenderer.vrf For details, refer to the Infor Reporting Designer User Guide.
Microsoft Reporting Services | Leave the path empty.
Change Output file allowed | If this check box is selected, you can change the default path and file at run time when you print to a file.
Page Length | If you send the output to a file, you can enter the page length for the output. Note You must also define the height of your screen display.