| # Reporting Line Station Order Complete Using Bar Code To report a line station order complete Step 1. Print the required codes Print the bar codes your require, with the Print Line Station Orders (Bar Code) (tiasc2411m000) session. You can keep a printout of the action bar codes by your scanner, and scan the assembly order numbers from labels attached to the orders. Step 2. Select the line station (optional) If you report a line station order Complete at a different line station, click the New Station button. Step 3. Scan the order code When the line station order is completed, scan the bar code on the order. The order number is displayed in the Assembly Order field. If the scanner cannot read the bar code, enter the number manually. Step 4. Scan the Complete code Scan the bar code for Complete. A code is displayed in the Action field. If the scanner cannot read the bar code, enter Complete manually. To enter this manually, enter the correct code and press the TAB key. To undo a reporting complete action Step 1. Scan the order code Scan the bar code on the order. Step 2. Scan the Undo Complete LSO code Scan the bar code for Undo complete LSO. Note You must set your bar code reader so that it adds a tab character at the end of each code. The code to Complete is 0001. The code to undo the Complete is 0002. The code to end the session without using the keyboard is 0009. You can also report line station orders complete (without using bar codes) from the appropriate menu of the Line Station - Assembly Orders (tiasl6510m000) session. Related topics Assembly control overview Bar codes for Windows NT |