| # Inspections (tscfg3600m000) Use this session to maintain inspection performed on serialized items. The session also provide data about the measurement that are recorded for the item inspected. The tabs refer to the following sessions: Maintenance Triggers: Maintenance Triggers (tsmdm0169m200) session. Maintenance Notifications: Maintenance Notifications (tscfg3110m000) session. Note Inspections can be performed on a service order, a work order or not based on an order. Related topics Service inspections and preventive maintenance scenarios Done For Business Object The order number for which the measurement is performed. Allowed values This field can have the following values Service Order Work Order Not Applicable Activity Line The activity line of the order on which the measurement is performed. Description The description or name of the code. Item The ID of the item for which inspection is performed. Serial Number The serial number of the item for which inspection is performed. Description The description or name of the code. Inspection Measurement Type The code of the measurement type. Description The description or name of the code. Position The position identification of the place where the item to be measured is located. Description The description or name of the code. Measured Value Numeric The measured value for the numeric measurement type. Unit The unit in which the measurement is expressed. Registration Expected Value The expected value based on the trend is defined in the counter reading. Unit The unit in which the expected value is expressed. Measured Value The measured value for the alphanumeric measurement type. Handled by The code of the service engineer who performed the measurement. Engineer Name The name of the service engineer who performed the measurement. Measured On The date and time when the actual measurement was performed. Creation Date The date and time the measurement is created or generated. Inspection Status The status of the inspection. Allowed values Inspection Status Text If this check box is selected, a text is present. Picture The picture of the item for which the inspection is performed. |