| # Inspection Orders (qmptc2100m100) Use this session to define and modify storage inspection orders for an item. Related topics Storage inspections Order An order used to structure the inspection of products that are purchased, produced, or sold. Standard Test Procedure The code to which data is linked that is necessary to check the quality requirements of an item. Since one standard test procedure can be used for a group of products that require the same quality standards and tests, a standard test procedure can considerably reduce time. Test Group The definition of how often you take samples to test an order quantity, and what the sample size is. Test Type Specification of how samples are taken from the order quantity. Allowed values Possible Values Frequency The interval between two samples, expressed in the frequency unit. Explanation: A new sample of 10 pieces is drawn for every 100 pieces. In this case there will be 11 samples of 10 pieces. Example
Sample | 10 pieces
Frequency | 100 pieces
Order quantity | 1150 pieces
Note You cannot continue the inspection procedure when your order quantity is less than the frequency quantity (for example, when your order quantity is 40, and your frequency quantity is 50). In such a case, no samples can be generated, and you must decrease the frequency quantity. Frequency Unit The unit in which the sample size is expressed. Note The frequency unit and the unit of the order quantity do not have to be identical. However, when they are not identical a correct conversion factor is essential. Percentage The sample size is the total quantity that is to be tested. In this field, the sample size is expressed as a percentage of either the order quantity or the frequency (in case you selected Continuous Sampling as the test type). Sample Size The sample size is the total quantity of all samples which are to be tested out of the order quantity, expressed in the unit of the sample size. In this field, it is expressed as a fixed quantity. Unit The unit of the sample size. Lines Click to start the Inspection Order Lines (qmptc1101m000) session. Samples Click to start the Inspection Order Samples (qmptc1110m000) session. |