| # Improved Component CTP offset If you perform a component CTP check, LN determines the date of the component requirement as part of the checking process. Infor LN FP5 In Infor LN FP5, this requirement date is always derived from the lead-time offset defined on the BOM line for the component. As a consequence, you have to define the lead-time offset on every BOM line where the component was used, or else the component CTP check will produce incorrect results. New in Infor LN FP6 In Infor LN FP6, if you clear the Use Lead Time Offset check box on the BOM line, LN uses the order lead time defined in the Items - Production (tiipd0101m000) session as lead-time offset in component CTP checks. For more information, refer to Component CTP. |