| # Automated communication Determine the networks that will have automated communication and their appropriate time intervals. You can define as many connect frequencies as necessary. The connection frequency determines when the Direct Network Communication (ecedi7205m000) session is started. Based on the frequencies, you can generate a list of individual connect times per network. Instead of having to maintain the next connect time with the Connect Times by Network (ecedi0125m000) session, ERP can calculate the connect times by using the data defined in the Connect Frequencies by Network (ecedi0122s000) session. The Generate Connect Times by Network (ecedi0225m000) session generates individual connect times. You can display or modify the result with the Connect Times by Network (ecedi0125m000) session. Related topics EDI interchange controller Communication |