| # Maintenance Triggers (tsmdm0169m000) Use this session to define numeric maintenance triggers for the maintenance trigger set. When you perform an inspection LN checks for an applicable maintenance trigger set. If the measured value meets with one of the maintenance triggers within the trigger set, a maintenance notification is generated. Related topics Service inspections and preventive maintenance scenarios Maintenance Trigger Set The maintenance triggers set to which the trigger belongs. Description The description or name of the code. Trigger Number The number of the maintenance trigger. Limit Value The limit of the maintenance trigger. Allowed values Limit value Lower Limit Value The value to specify the limit from when maintenance must be triggered. Upper Limit Value The value to specify the limit up to which maintenance must be triggered. Unit The unit of the limit value. Limit Period The time period when the trigger is valid. Allowed values Limit Period Lower Limit Period Value The time period from when the trigger is valid. Upper Limit Period Value The time period up to which the trigger is valid. Limit Period Unit The unit of the limit period. Allowed values Unit Trigger Message The code of the trigger message. Description The description or name of the code. Default Recommendation The recommendation defined as the default value for the maintenance trigger. LN defaults the value only if the Default check box is selected in the Recommendations (tsmdm0167m000) session. Description The description or name of the code. Default Follow-up Activity The reference activity defined as the default follow-up activity of the maintenance notification. LN defaults the default Follow-up Activity from the Recommendations (tsmdm0167m000) session. Description The description or name of the code. |